#ISD App Configuration:3.1
# ISD version: 4.21.0.qualifier
#  Directory of framework within the stack, which helps in case there are more
#  frameworks within a stack.
FrameworkDirectory:app/framework

#  Identified of a stack descriptor used for this configuration. This should not
#  be changed manually, unless you really know what you are doing.
ConfiguratorID:auto-EM35XEZSP

#  Output directory which is used as a root for all generated files. The actual
#  files relative to that directory are defined by individual file name.
GenerationDirectory:__SAMPLE_APPLICATION__

#  Unique identifier for this device. This string should be in a form of a C
#  identifier, as it will be used in both generated variable, macros, as well as
#  file names. You should generally not use characters which are not valid
#  characters in a C identifier here.
DeviceName:SwitchedMultiprotocolTrustCenter

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Primary,0

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Primary,HA-onoff

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Centralized,80

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Centralized,HA-homegatewayems

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Touchlink,512

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Touchlink,ZLL-colorlight

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:GreenPower,96

#  The ZCL device that this particular endpoint is implementing.
DeviceType:GreenPower,GP-proxy

#  ZigBee PRO network configuration.  Each endpoint belongs to a single network
#  configuration.  There can be one or more network configurations.
ZigbeeProNetwork:*Primary,ZA_COORDINATOR,Z3

#  Lists the channels that this application will be configured to use.
Channels:11

#  Definitions of individual endpoints. For each endpoint the endpoint number
#  (1-254) is listed, as well as the endpoint type that this endpoint will
#  serve.
ConfiguredEndpoints:*1&-1&-1&0&Centralized&Primary,242&-1&-1&0&GreenPower&Primary

#  A single specification version for each profile defining the max version of
#  the spec supported by this configuration.
SpecVersions:

#  In case of a network coprocessor, this lists a host processor used.
Host:pc

#  Ember network processor targeted for this application.
Platform:pc

#  Enable callbacks.
Callbacks:emberAfHalButtonIsrCallback,

#  Any customer-specific general purpose custom events.
CustomEvents:commissioningEventControl,commissioningEventHandler

#  If bindings are enabled then this is the maximum number of supported
#  bindings.
NumberOfBindings:2

#  The size of the stack address table which will be used by the stack to
#  maintain IEEE to ZigBee short id mappings.
AddressTableSize:2

#  The size of the portion of the address table used by the trust center as an
#  address cache. The total size of the address table will be equal to this
#  value plus the size of the address table set in the AddressTableSize.
TrustCenterCacheSize:2

#  Maximum number of supported reported attributes.
ReportTableSize:5

#  The mode of the link key handling on a trust center.
LinkKeyMode:2

#  If not using multiple endpoint support, this value contains the default
#  endpoint. With multiple endpoint support, this number is ignored.
Endpoint:10

#  Version of this device.
DeviceVersion:0

#  Master endpoint which contains global information.
DefaultDestinationEndpoint:10

#  Profile Id used for the application.
ProfileId:-1

#  Device Id used for the application.
DeviceId:-1

#  The largest size for a fragment buffer.
FragmentationMaxSize:255

#  Size of the table for source routing.
SourceRouteTableSize:7

#  The level of debugging supported.
DebugLevel:1

#  Configuration of command-line interface.
CLIMode:2

#  Configuration of heartbeat.
HeartbeatLed:2

#  If this option is set to true, standard reporting is enabled.
EnableStandardReporting:false

#  If the device needs to perform inter-PAN sends, then this option should be
#  enabled.
EnableInterPanSend:false

#  If the device needs to perform inter-PAN receives, then this option should be
#  enabled.
EnableInterPanReceive:false

#  Enable serial commands for ZDO.
EnableZdoSerialCommands:false

#  Enable this option if you wish to enable device bindings.
EnableBindings:true

#  Turn this option on, if end-device binding is enabled.
EnableEndDeviceBind:false

#  Enables the statistics receiving.
EnableReceiveStatistics:false

#  If true, then command discovery commands are supported.
SupportCommandDiscovery:true

#  Selects whether application will use the ECC 163k1 library.
UseEcc163k1:false

#  Selects whether application will use the ECC 283k1 library.
UseEcc283k1:false

#  Enable preconfigured keys for security.
PreconfiguredKeyEnabled:false

#  Enable network key.
NetworkKeyEnabled:false

#  If this option is turned on, then appBuilder will automatically generate the
#  files, immediately upon saving the ISC file.
AutoGenerate:false

#  Enable key switching.
EnableKeySwitch:false

#  Use this setting to turn on fragmentation.
FragmentationEnable:false

#  Enables concentrator support
EnableConcentrator:true

#  If true, then this concentrator is low ram, otherwise high ram
LowRamConcentrator:true

#  If this option is set to true, then MFG_INSTALL_CODE token is used for
#  setting the security install code.
UseSeInstallCodes:false

#  If this option is turned on, then the code will enable the checking of the
#  attributes.
EnableAttributeRangeChecking:false

#  Enable application handling of supported ZigBee Device Object messages.
ReceiveSupportedZdoRequests:false

#  Enable application handling of unsupported ZigBee Device Object messages.
HandleUnsupportedZdoRequests:false

#  Enable application handling of ZigBee Device Object requests related to
#  endpoints.
HandleEndpointZdoRequests:false

#  Enable application handling of ZigBee Device Object requests related to
#  bindings.
HandleBindingZdoRequests:false

#  Use token for TX power mode.
TxPowerModeUseToken:true

#  Enable boost power mode.
BoostMode:false

#  Enable the alternate transmitter output.
AlternatePowerMode:false

#  Use legacy CLI instead of generated CLI.
LegacyCli:false

#  Add Custom CLI sub-menu
AddCustomCli:false

#  Include command and argument descriptions in the embedded code.
IncludeCommandDescriptions:true

#  If set, then project-specific callbacks file will be generated.
GenerateCallbacksFile:false

#  The manufacturer code for this app defaults to 0.
ManufacturerCodeDefaultIsZero:true

#  Actual preconfigured key, if it is enabled.
PreconfiguredKey:56777777777777777777777777777777

#  Actual network key.
NetworkKey:12333333333333333333333333333333

#  Actual second network key.
NetworkKey2:ABCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC


# Setup configurations
{setupId:additionalFiles
}
{setupId:boardHeader
allowMissingHeader:false
useHeaderInPlace:false
}
{setupId:bookkeeping
}
{setupId:bootloader
}
{setupId:callbackConfiguration
}
{setupId:debugConfiguration
on
area name off
appSerial=1
}
{setupId:halOptions
}
{setupId:hwConfig
featureLevel=1
active=true
}
{setupId:information
\{key:description
Switched Multiprotocol Sample Applications

The switched multiprotocol applications demonstrate the switched multiprotcol
feature from Silabs. These applications showcase the commissioning mechanism
via the MPSI protocol and the ability to load other stacks in storage.

The SwitchedMultiprotocolZ3Gateway application is effectively a Z3Gateway
application. To the difference of the Z3Gateway application, it adds support for
switched multiprotocol by adding the necessary plugins. Like the Z3Gatway
application, it forms a network using the Network Creator plugin when button 0
is pressed. Permitting joining, however, is now only controlled by MPSI messages
(or by CLI commands).

The SwitchedMultiprotocolZ3Light application is a Z3Light application with added
switched multiprotocol support. To the difference of the Z3Light application, it
does not try to join a network after booting. Instead, network joining is
controlled by MPSI messages (or by CLI commands).

These applications are intended to be configured with the use of a mobile
application. The mobile application probes and configures the devices over a
bluetooth connection.

A piece of metadata be added to an application to convey the maximum MPSI
message ID supported. This metadata is supplied to commander when creating a GBL
from the application binary. The file mpsi-metadata.bin is provided as the
metadata needed to convey max MPSI message ID supported. A GBL that conveys this
MPSI message ID limit can be created with the following command.

commander gbl create \\{desired gbl name\\} --app \\{application binary\\} --metadata
 mpsi/mpsi-metadata.bin

The resulting GBL can then be loaded onto external flash or internal flash,
which can then be inspected by a running application for the maximum understood
MPSI message ID.

This procedure does not apply to host images since they do not wrap into a GBL.
\}
}
{setupId:macros
}
{setupId:mpsi
- mappings
- custom messages
}
{setupId:quizz
}
{setupId:serial
em317=0,false,*,*,*,*,*
em341=0,false,*,*,*,*,*
em342=0,false,*,*,*,*,*
em346=0,false,*,*,*,*,*
em351=0,false,*,*,*,*,*
em355=0,false,*,*,*,*,*
em3555=0,false,*,*,*,*,*
em357=0,false,*,*,*,*,*
em357p2p=0,false,*,*,*,*,*
em3581=0,false,*,*,*,*,*
em3582=0,false,*,*,*,*,*
em3585=0,false,*,*,*,*,*
em3586=0,false,*,*,*,*,*
em3587=0,false,*,*,*,*,*
em3588=0,false,*,*,*,*,*
em3591=0,false,*,*,*,*,*
em3592=0,false,*,*,*,*,*
em3595=0,false,*,*,*,*,*
em3596=0,false,*,*,*,*,*
em3597=0,false,*,*,*,*,*
em3598=0,false,*,*,*,*,*
sky66107=0,false,*,*,*,*,*
simulation=0,false,*,*,*,*,*
efr32=0,false,*,*,*,*,*
useHwConfigurator=false
}
{setupId:token
}
#  The name of the set of Command Line Interface (CLI) commands that are
#  compiled into the application by default.
CliCommandSet:Full

#  These are the various Command Line Interface (CLI) commands that can be
#  included, or excluded (if they are included by default), in the application.
#  Plugin configuration
appPlugin:address-table,true

appPlugin:aes-cmac,false

appPlugin:basic,true

appPlugin:button-joining,false

appPlugin:calendar-client,true

appPlugin:calendar-common,false

appPlugin:calendar-server,true

appPlugin:color-control,true

appPlugin:color-control-server,false

appPlugin:command-relay,false

appPlugin:comms-hub-function,false

appPlugin:concentrator,true

appPlugin:counters,true

appPlugin:device-database,false

appPlugin:device-management-client,false

appPlugin:device-management-server,false

appPlugin:device-query-service,false

appPlugin:device-table,false

appPlugin:diagnostic-server,true

appPlugin:door-lock-server,false

appPlugin:drlc,true

appPlugin:drlc-server,false

appPlugin:ember-minimal-printf,false

appPlugin:end-device-support,false

appPlugin:esi-management,true

appPlugin:events-client,false

appPlugin:events-server,false

appPlugin:exosite-demo,false

appPlugin:ezmode-commissioning,false

appPlugin:find-and-bind-initiator,false

appPlugin:find-and-bind-target,false

appPlugin:form-and-join,false

appPlugin:fragmentation,false

appPlugin:gas-proxy-function,false

appPlugin:gbcs-device-log,false

appPlugin:gbcs-gas-meter,false

appPlugin:gbz-message-controller,false

appPlugin:general-response-commands,false

appPlugin:green-power-client,true

appPlugin:green-power-common,true

appPlugin:green-power-server,false

appPlugin:green-power-test-device,false

appPlugin:groups-client,false

appPlugin:groups-server,true

appPlugin:hc-11073-tunnel,true

appPlugin:heartbeat,true

appPlugin:ias-zone-client,false

appPlugin:ias-zone-server,false

appPlugin:identify,true

appPlugin:identify-feedback,false

appPlugin:infrared-led,false

appPlugin:interpan,false

appPlugin:key-establishment,true

appPlugin:level-control,true

appPlugin:lwip,false

appPlugin:lwip-callback-tests,false

appPlugin:lwip-interface,false

appPlugin:lwip-stats,false

appPlugin:lwip-udp-wrapper,false

appPlugin:manufacturing-library-cli,false

appPlugin:messaging-client,true

appPlugin:messaging-server,true

appPlugin:meter-mirror,false

appPlugin:meter-snapshot-client,false

appPlugin:meter-snapshot-server,false

appPlugin:meter-snapshot-storage,false

appPlugin:mn-price-passthrough,false

appPlugin:network-creator,true

appPlugin:network-creator-security,true

appPlugin:network-find,false

appPlugin:network-steering,false

appPlugin:on-off,true

appPlugin:ota-bootload,true

appPlugin:ota-client,true

appPlugin:ota-client-policy,true

appPlugin:ota-common,true

appPlugin:ota-server,true

appPlugin:ota-server-policy,true

appPlugin:ota-storage-common,false

appPlugin:ota-storage-posix-filesystem,false

appPlugin:ota-storage-simple,false

appPlugin:ota-storage-simple-eeprom,false

appPlugin:ota-storage-simple-ram,false

appPlugin:partner-link-key-exchange,true

appPlugin:permit-join-manager,false

appPlugin:poll-control-client,true

appPlugin:poll-control-server,true

appPlugin:power-consumption-model,false

appPlugin:prepayment-client,false

appPlugin:prepayment-server,false

appPlugin:prepayment-snapshot-storage,false

appPlugin:price-client,true

appPlugin:price-common,false

appPlugin:price-server,true

appPlugin:reporting,false

appPlugin:scan-dispatch,true

appPlugin:scenes,true

appPlugin:scenes-client,false

appPlugin:simple-clock,false

appPlugin:simple-main,true

appPlugin:simple-metering-client,false

appPlugin:simple-metering-server,true

appPlugin:sleepy-message-queue,false

appPlugin:smart-energy-registration,false

appPlugin:stack-diagnostics,false

appPlugin:standalone-bootloader-client,false

appPlugin:standalone-bootloader-common,false

appPlugin:standalone-bootloader-server,false

appPlugin:standard-printf-support,false

appPlugin:sub-ghz-client,false

appPlugin:sub-ghz-server,false

appPlugin:test-harness,false

appPlugin:test-harness-z3,false

appPlugin:throughput,false

appPlugin:throughput-library,false

appPlugin:time-server,true

appPlugin:trust-center-backup,false

appPlugin:trust-center-keepalive,false

appPlugin:trust-center-nwk-key-update-broadcast,false

appPlugin:trust-center-nwk-key-update-periodic,false

appPlugin:trust-center-nwk-key-update-unicast,false

appPlugin:tunneling-client,true

appPlugin:tunneling-server,true

appPlugin:update-tc-link-key,false

appPlugin:xmodem-sender,false

appPlugin:zcl-ip,false

appPlugin:zll-commissioning,false

appPlugin:zll-identify-server,false

appPlugin:zll-level-control-server,false

appPlugin:zll-on-off-server,false

appPlugin:zll-scenes-client,false

appPlugin:zll-scenes-server,false

appPlugin:zll-utility-client,false

appPlugin:zll-utility-server,false

appPlugin:aes-software,false

appPlugin:coap-server,false

appPlugin:custom-ezsp,false

appPlugin:ezsp,true

appPlugin:ezsp-spi,false

appPlugin:ezsp-uart,true

appPlugin:ezsp-usb,false

appPlugin:file-descriptor-dispatch,true

appPlugin:gateway,true

appPlugin:gateway-relay-coap,false

appPlugin:gateway-relay-mqtt,false

appPlugin:ncp-configuration,true

appPlugin:secure-ezsp,false

appPlugin:secure-ezsp-stub,true

appPlugin:security-support,false

appPlugin:unix-library,true

appPlugin:unix-printf,true

appPlugin:mpsi,true

appPlugin:battery-monitor,false

appPlugin:battery-monitor-stub,false

appPlugin:bulb-pwm-driver,false

appPlugin:button-interface,false

appPlugin:button-interface-stub,false

appPlugin:eeprom,false

appPlugin:generic-interrupt-control,false

appPlugin:generic-interrupt-control-stub,false

appPlugin:gpio-sensor,false

appPlugin:gpio-sensor-stub,false

appPlugin:led-blink,false

appPlugin:led-blink-stub,false

appPlugin:occupancy-pyd1698,false

appPlugin:occupancy-pyd1698-stub,false

appPlugin:power-meter-cs5463,false

appPlugin:power-meter-cs5463-stub,false

appPlugin:sb1-gesture-sensor,false

appPlugin:sb1-gesture-sensor-stub,false

appPlugin:tamper-switch,false

appPlugin:tamper-switch-stub,false

appPlugin:linked-list,false

appPlugin:module-lna,false

appPlugin:mpsi-ipc,true

appPlugin:mpsi-storage,false

appPlugin:transport-mqtt,false

appPlugin:slot-manager,false

appPlugin:cjson,false

appPlugin:libcoap,false

appPlugin:paho.mqtt.c,false

