#ISD afv6
# Simplicity Studio version: 4.29.1.qualifier

# Application configuration
appId: ncp
frameworkRoot: app/ncp
architecture: em357+iar
deviceName: ncp-uart-sw
generationDirectory: PATH(ISC_RELATIVE):.

# Devices

# Plugin configuration
appPlugin: accelerometer-led=false
appPlugin: adc=true
appPlugin: antenna=false
appPlugin: antenna-stub=true
appPlugin: battery-monitor=false
appPlugin: binding-table-library=true
appPlugin: binding-table-stub-library=false
appPlugin: bulb-pwm-driver=false
appPlugin: button=false
appPlugin: button-interface=false
appPlugin: button-stub=true
appPlugin: buzzer=false
appPlugin: buzzer-stub=true
appPlugin: cbke-163k1-library=false
appPlugin: cbke-163k1-stub-library=true
appPlugin: cbke-283k1-library=false
appPlugin: cbke-283k1-stub-library=true
appPlugin: cbke-library-core=false
appPlugin: cbke-library-dsa-sign=false
appPlugin: cbke-library-dsa-sign-stub=true
appPlugin: cbke-library-dsa-verify=false
appPlugin: cbke-library-dsa-verify-283k1=false
appPlugin: cbke-library-dsa-verify-283k1-stub=true
appPlugin: cbke-library-dsa-verify-stub=true
appPlugin: cbke-stub-library=true
appPlugin: cjson=false
appPlugin: coexistence=true
appPlugin: coexistence-stub=false
appPlugin: concentrator-support-library=true
appPlugin: concentrator-support-stub-library=false
appPlugin: debug-basic-library=true
appPlugin: debug-basic-stub-library=false
appPlugin: debug-channel=true
appPlugin: debug-channel-stub=false
appPlugin: debug-extended-library=true
appPlugin: debug-extended-stub-library=false
appPlugin: diagnostic=true
appPlugin: diagnostic-stub=false
appPlugin: dmp-demo-ui=false
appPlugin: ecc-library-163k1=false
appPlugin: ecc-library-283k1=false
appPlugin: eeprom=false
appPlugin: eeprom-powerdown=false
appPlugin: ember-minimal-printf=true
appPlugin: end-device-bind-library=true
appPlugin: end-device-bind-stub-library=false
appPlugin: ext-device=true
appPlugin: extdev=false
appPlugin: ezradiopro=false
appPlugin: ezsp-binding=true
appPlugin: ezsp-cbke=true
appPlugin: ezsp-gp=true
appPlugin: ezsp-mfglib=true
appPlugin: ezsp-security=true
appPlugin: ezsp-zigbee-pro=true
appPlugin: ezsp-zll=true
appPlugin: fem-control=false
appPlugin: generic-interrupt-control=false
appPlugin: glib=false
appPlugin: gp-library=true
appPlugin: gp-stub-library=false
appPlugin: gpio-sensor=false
appPlugin: hal-library=true
appPlugin: heartbeat=false
appPlugin: humidity-si7021-stub=false
appPlugin: i2c-driver=false
appPlugin: i2c-driver-stub=false
appPlugin: illuminance-si1141-stub=false
appPlugin: install-code-library=true
appPlugin: install-code-library-stub=false
appPlugin: key-matrix=false
appPlugin: led=true
appPlugin: led-blink=false
appPlugin: led-stub=false
appPlugin: libcoap=false
appPlugin: linked-list=false
appPlugin: mfglib-library=true
appPlugin: mfglib-stub-library=false
appPlugin: microphone-codec-msadpcm=false
appPlugin: microphone-imaadpcm=false
appPlugin: mpsi=false
appPlugin: mpsi-ipc=false
appPlugin: mpsi-storage=false
appPlugin: multi-network-library=false
appPlugin: multi-network-stub-library=true
appPlugin: ncp-spi=false
appPlugin: ncp-uart=true
appPlugin: ncp-usb=false
appPlugin: occupancy-pyd1698=false
appPlugin: occupancy-pyd1698-stub=false
appPlugin: pa=false
appPlugin: packet-validate-library=true
appPlugin: packet-validate-stub-library=false
appPlugin: paho.mqtt.c=false
appPlugin: power-meter-cs5463=false
appPlugin: psstore=false
appPlugin: pti=false
appPlugin: rail-library=true
appPlugin: rail-library-mp=false
appPlugin: sb1-gesture-sensor=false
appPlugin: secure-ezsp=false
appPlugin: secure-ezsp-stub=true
appPlugin: security-library-core=true
appPlugin: security-library-link-keys=true
appPlugin: security-library-link-keys-stub=false
appPlugin: serial=true
appPlugin: sim-eeprom1=false
appPlugin: sim-eeprom2=true
appPlugin: sim-eeprom2-1to2-upgrade=false
appPlugin: sim-eeprom2-1to2-upgrade-stub=true
appPlugin: slot-manager=false
appPlugin: stm32f103ret-library=false
appPlugin: stub-security-library=false
appPlugin: tamper-switch=false
appPlugin: temperature-si7053-stub=false
appPlugin: transport-mqtt=false
appPlugin: unix-library=false
appPlugin: xncp=false
appPlugin: xncp-stub=true
appPlugin: zigbee-pro-leaf-library=false
appPlugin: zigbee-pro-stack=true
appPlugin: zigbee-r22-support-library=false
appPlugin: zigbee-r22-support-stub-library=true
appPlugin: zll-library=true
appPlugin: zll-stub-library=false

# Setup configurations
{setupId:additionalFiles
}
{setupId:boardHeader
allowMissingHeader:false
useHeaderInPlace:false
EFR32MG1P132F256GM48=BOARD,efr32/brd4153a,,
EFR32MG1P232F256GM48=BOARD,efr32/brd4151a,,
EFR32MG1P233F256GM48=BOARD,efr32/brd4150a,,
em355=BOARD,em35x/dev0680uart_21gpio,,
em3555=BOARD,em35x/dev0680uart_21gpio,,
em357=BOARD,em35x/dev0680uart,,
em3581=BOARD,em35x/dev0680uart,,
em3582=BOARD,em35x/dev0680uart,,
em3585=BOARD,em35x/dev0680uart,,
em3586=BOARD,em35x/dev0680uart,,
em3587=BOARD,em35x/dev0680uart,,
em3588=BOARD,em35x/dev0680uart,,
em3591=BOARD,em35x/ncp_uart_sc1,,
em3592=BOARD,em35x/ncp_uart_sc1,,
em3595=BOARD,em35x/ncp_uart_sc1,,
em3596=BOARD,em35x/ncp_uart_sc1,,
em3597=BOARD,em35x/ncp_uart_sc1,,
em3598=BOARD,em35x/ncp_uart_sc1,,
}
{setupId:bookkeeping
}
{setupId:bootloader
}
{setupId:callbackConfiguration
emberAfEzspClearBindingTableCommandCallback:true
emberAfEzspSetBindingCommandCallback:true
emberAfEzspGetBindingCommandCallback:true
emberAfEzspDeleteBindingCommandCallback:true
emberAfEzspBindingIsActiveCommandCallback:true
emberAfEzspGetBindingRemoteNodeIdCommandCallback:true
emberAfEzspSetBindingRemoteNodeIdCommandCallback:true
emberAfEzspRemoteSetBindingHandlerCommandCallback:true
emberAfEzspRemoteDeleteBindingHandlerCommandCallback:true
}
{setupId:eventConfiguration
}
{setupId:ezsp
}
{setupId:genConfig
}
{setupId:halOptions
}
{setupId:hwConfig
featureLevel=1
active=true
}
{setupId:information
\{key:description
NCP UART Application

This network coprocessor (NCP) application supports communication with a host application over a UART interface with software flow control. This NCP application can be built as configured, or optionally can be augmented with customizations for target hardware, initialization, main loop processing, event definition/handling, and messaging with the host.

As configured, this NCP UART application is the basis for building the corresponding binary ncp-uart images delivered with the Silicon Labs zigbee stack.

Refer to the Silicon Labs zigbee documentation for more information about NCP customization.
\}
}
{setupId:macros
}
{setupId:quizz
}
{setupId:serial
useHwConfigurator=false
}
{setupId:template
simeepromSize=36864
}
{setupId:token
}

# Plugin options
pluginOption(simulation): EMBER_PACKET_BUFFER_COUNT,64
pluginOption(simulation): EMBER_AF_PLUGIN_ZIGBEE_PRO_STACK_CHILD_TABLE_SIZE,32
pluginOption(simulation): EMBER_AF_PLUGIN_SIM_EEPROM2_PASSWORD,!spoon
pluginOption(simulation): EMBER_MAX_END_DEVICE_CHILDREN,32
pluginOption(simulation): EMBER_BINDING_TABLE_SIZE,32
pluginOption(simulation): EMBER_KEY_TABLE_SIZE,12
pluginOption(efr32): EMBER_AF_PLUGIN_NCP_UART_FLOW_CONTROL,Software
pluginOption(efr32): EMBER_AF_PLUGIN_HAL_CONFIG_VUART_ENABLE,1
pluginOption(efr32~device_configuration[1]): EMBER_AF_PLUGIN_HAL_CONFIG_USART0_FLOW_CONTROL,HAL_USART_FLOW_CONTROL_SW
pluginOption(efr32~device_configuration[3]): EMBER_AF_PLUGIN_HAL_CONFIG_USART0_FLOW_CONTROL,HAL_USART_FLOW_CONTROL_SW
pluginOption(efr32~device_configuration[2]): EMBER_AF_PLUGIN_HAL_CONFIG_USART0_ENABLE,0
pluginOption(efr32~device_configuration[2]): EMBER_AF_PLUGIN_HAL_CONFIG_USART0_FLOW_CONTROL,HAL_USART_FLOW_CONTROL_NONE
pluginOption(efr32~device_configuration[2]): EMBER_AF_PLUGIN_HAL_CONFIG_USART3_ENABLE,1
pluginOption(efr32~device_configuration[2]): EMBER_AF_PLUGIN_HAL_CONFIG_USART3_FLOW_CONTROL,HAL_USART_FLOW_CONTROL_SW
