#ISD afv6
# Simplicity Studio version: 4.29.1.qualifier

# Application configuration
appId: ncp
frameworkRoot: app/ncp
architecture: efr32~family[M]~series[1]~device_configuration[1]~performance[P]~radio[132]~flash[256K]~temp[G]~package[M]~pins[48]+BRD4155A+iar
deviceName: xncp-commshub-uart-dual
generationDirectory: PATH(ISC_RELATIVE):.

# Devices

# Plugin configuration
appPlugin: accelerometer-led=false
appPlugin: adc=true
appPlugin: antenna=false
appPlugin: antenna-stub=true
appPlugin: battery-monitor=false
appPlugin: binding-table-library=true
appPlugin: binding-table-stub-library=false
appPlugin: bulb-pwm-driver=false
appPlugin: button=false
appPlugin: button-interface=false
appPlugin: button-stub=true
appPlugin: buzzer=false
appPlugin: buzzer-stub=false
appPlugin: cbke-163k1-library=false
appPlugin: cbke-163k1-stub-library=true
appPlugin: cbke-283k1-library=false
appPlugin: cbke-283k1-stub-library=true
appPlugin: cbke-library-core=false
appPlugin: cbke-library-dsa-sign=false
appPlugin: cbke-library-dsa-sign-stub=true
appPlugin: cbke-library-dsa-verify=false
appPlugin: cbke-library-dsa-verify-283k1=false
appPlugin: cbke-library-dsa-verify-283k1-stub=true
appPlugin: cbke-library-dsa-verify-stub=true
appPlugin: cbke-stub-library=true
appPlugin: cjson=false
appPlugin: coexistence=true
appPlugin: coexistence-stub=false
appPlugin: concentrator-support-library=true
appPlugin: concentrator-support-stub-library=false
appPlugin: debug-basic-library=true
appPlugin: debug-basic-stub-library=false
appPlugin: debug-channel=true
appPlugin: debug-channel-stub=false
appPlugin: debug-extended-library=true
appPlugin: debug-extended-stub-library=false
appPlugin: diagnostic=true
appPlugin: diagnostic-stub=false
appPlugin: dmp-demo-ui=false
appPlugin: ecc-library-163k1=false
appPlugin: ecc-library-283k1=false
appPlugin: eeprom=false
appPlugin: eeprom-powerdown=false
appPlugin: ember-minimal-printf=true
appPlugin: end-device-bind-library=true
appPlugin: end-device-bind-stub-library=false
appPlugin: ext-device=true
appPlugin: extdev=false
appPlugin: ezradiopro=false
appPlugin: ezsp-binding=true
appPlugin: ezsp-cbke=true
appPlugin: ezsp-gp=false
appPlugin: ezsp-mfglib=true
appPlugin: ezsp-security=true
appPlugin: ezsp-zigbee-pro=true
appPlugin: ezsp-zll=false
appPlugin: fem-control=false
appPlugin: generic-interrupt-control=false
appPlugin: glib=false
appPlugin: gp-library=false
appPlugin: gp-stub-library=true
appPlugin: gpio-sensor=false
appPlugin: hal-library=true
appPlugin: heartbeat=true
appPlugin: humidity-si7021-stub=false
appPlugin: i2c-driver=false
appPlugin: i2c-driver-stub=false
appPlugin: illuminance-si1141-stub=false
appPlugin: install-code-library=true
appPlugin: install-code-library-stub=false
appPlugin: key-matrix=false
appPlugin: led=true
appPlugin: led-blink=false
appPlugin: led-stub=false
appPlugin: libcoap=false
appPlugin: linked-list=false
appPlugin: mfglib-library=true
appPlugin: mfglib-stub-library=false
appPlugin: microphone-codec-msadpcm=false
appPlugin: microphone-imaadpcm=false
appPlugin: mpsi=false
appPlugin: mpsi-ipc=false
appPlugin: mpsi-storage=false
appPlugin: multi-network-library=false
appPlugin: multi-network-stub-library=true
appPlugin: ncp-spi=false
appPlugin: ncp-uart=true
appPlugin: ncp-usb=false
appPlugin: occupancy-pyd1698=false
appPlugin: occupancy-pyd1698-stub=false
appPlugin: pa=true
appPlugin: packet-validate-library=true
appPlugin: packet-validate-stub-library=false
appPlugin: paho.mqtt.c=false
appPlugin: power-meter-cs5463=false
appPlugin: psstore=false
appPlugin: pti=true
appPlugin: rail-library=true
appPlugin: rail-library-mp=false
appPlugin: sb1-gesture-sensor=false
appPlugin: secure-ezsp=false
appPlugin: secure-ezsp-stub=true
appPlugin: security-library-core=true
appPlugin: security-library-link-keys=true
appPlugin: security-library-link-keys-stub=false
appPlugin: serial=true
appPlugin: sim-eeprom1=true
appPlugin: sim-eeprom2=false
appPlugin: sim-eeprom2-1to2-upgrade=false
appPlugin: sim-eeprom2-1to2-upgrade-stub=true
appPlugin: slot-manager=false
appPlugin: stm32f103ret-library=false
appPlugin: stub-security-library=false
appPlugin: tamper-switch=false
appPlugin: temperature-si7053-stub=false
appPlugin: transport-mqtt=false
appPlugin: unix-library=false
appPlugin: xncp=false
appPlugin: xncp-stub=true
appPlugin: zigbee-pro-leaf-library=false
appPlugin: zigbee-pro-stack=true
appPlugin: zigbee-r22-support-library=true
appPlugin: zigbee-r22-support-stub-library=false
appPlugin: zll-library=false
appPlugin: zll-stub-library=true

# Setup configurations
{setupId:additionalFiles
}
{setupId:boardHeader
allowMissingHeader:true
useHeaderInPlace:false
EFR32MG1P132F256GM48+BRD4155A=USE_HARDWARE_CONFIGURATOR,,,
efr32~family[M]~series[1]~device_configuration[1]~performance[P]~radio[132]~flash[256K]~temp[G]~package[M]~pins[48]+BRD4155A+iar=USE_HARDWARE_CONFIGURATOR,,,
}
{setupId:bookkeeping
}
{setupId:bootloader
}
{setupId:callbackConfiguration
}
{setupId:eventConfiguration
}
{setupId:ezsp
}
{setupId:halOptions
}
{setupId:hwConfig
lastArchitectureId=efr32~family[M]~series[1]~device_configuration[1]~performance[P]~radio[132]~flash[256K]~temp[G]~package[M]~pins[48]+BRD4155A+iar
featureLevel=1
active=true
}
{setupId:information
\{key:description
This is a demo network coprocessor application for a simultaneous dual phy device (2.4Ghz and subghz) that communicates to a host application over a UART interface. This application does not include ECC libraries. If you want to create an application with ECC support select cbke core, cbke 163k and cbke 283k libraries and add dependent libraries as per configuration error window if any.
\}
}
{setupId:macros
}
{setupId:quizz
q1=a3
}
{setupId:serial
useHwConfigurator=true
}
{setupId:template
simeepromSize=8192
}
{setupId:token
}

# Plugin options
pluginOption(): EMBER_AF_PLUGIN_SIM_EEPROM2_PASSWORD,!spoon
pluginOption(): EMBER_BINDING_TABLE_SIZE,32
