#ISD App Configuration:3.1
# ISD version: 4.21.0.qualifier
#  Identified of a stack descriptor used for this configuration. This should not
#  be changed manually, unless you really know what you are doing.
ConfiguratorID:auto-EM35X

#  Output directory which is used as a root for all generated files. The actual
#  files relative to that directory are defined by individual file name.
GenerationDirectory:__SAMPLE_APPLICATION__

#  Unique identifier for this device. This string should be in a form of a C
#  identifier, as it will be used in both generated variable, macros, as well as
#  file names. You should generally not use characters which are not valid
#  characters in a C identifier here.
DeviceName:DynamicMultiprotocolDemoSwitchWithNvm3

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Primary,0

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Primary,HA-onoff

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Touchlink,2080

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Touchlink,ZLL-noncolorremote

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Centralized,0

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Centralized,HA-onoff

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Green Power,97

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Green Power,GP-proxy-basic

#  ZigBee PRO network configuration.  Each endpoint belongs to a single network
#  configuration.  There can be one or more network configurations.
ZigbeeProNetwork:*Primary,ZA_ROUTER,Z3

#  Lists the channels that this application will be configured to use.
Channels:11

#  Definitions of individual endpoints. For each endpoint the endpoint number
#  (1-254) is listed, as well as the endpoint type that this endpoint will
#  serve.
ConfiguredEndpoints:*1&-1&-1&0&Centralized&Primary,2&-1&-1&0&Touchlink&Primary,242&-1&-1&0&Green Power&Primary

#  A single specification version for each profile defining the max version of
#  the spec supported by this configuration.
SpecVersions:

#  In case of a network coprocessor, this lists a host processor used.
Host:unknown

#  Ember network processor targeted for this application.
Platform:efr32~family[M]~series[1]~device_configuration[2]~performance[P]~radio[332]~flash[1024K]~temp[G]~package[L]~pins[125]+BRD4162A+iar

#  Enable callbacks.
Callbacks:emberAfHalButtonIsrCallback,emberAfStackStatusCallback,emberAfPluginFindAndBindInitiatorCompleteCallback,emberAfPluginNetworkSteeringCompleteCallback,emberAfPluginZllCommissioningTouchLinkCompleteCallback,emberAfPluginZllCommissioningTouchLinkFailedCallback,emberAfMainInitCallback,emberAfMainTickCallback,emberAfReportAttributesCallback,emberAfPreZDOMessageReceivedCallback,

#  Any customer-specific general purpose custom events.
CustomEvents:commissioningEventControl,commissioningEventHandler

CustomEvents:buttonEventControl,buttonEventHandler

CustomEvents:lcdMainMenuDisplayEventControl,lcdMainMenuDisplayEventHandler

CustomEvents:lcdPermitJoinEventControl,lcdPermitJoinEventHandler

#  If bindings are enabled then this is the maximum number of supported
#  bindings.
NumberOfBindings:2

#  The size of the stack address table which will be used by the stack to
#  maintain IEEE to ZigBee short id mappings.
AddressTableSize:2

#  The size of the portion of the address table used by the trust center as an
#  address cache. The total size of the address table will be equal to this
#  value plus the size of the address table set in the AddressTableSize.
TrustCenterCacheSize:2

#  Manufacturing code user in reporting.
ManufacturingCode:4098

#  Maximum number of supported reported attributes.
ReportTableSize:5

#  The mode of the link key handling on a trust center.
LinkKeyMode:2

#  If not using multiple endpoint support, this value contains the default
#  endpoint. With multiple endpoint support, this number is ignored.
Endpoint:10

#  Version of this device.
DeviceVersion:0

#  Master endpoint which contains global information.
DefaultDestinationEndpoint:10

#  Profile Id used for the application.
ProfileId:-1

#  Device Id used for the application.
DeviceId:-1

#  The largest size for a fragment buffer.
FragmentationMaxSize:255

#  Size of the table for source routing.
SourceRouteTableSize:7

#  Default response policy.
DefaultResponsePolicy:0

#  The level of debugging supported.
DebugLevel:1

#  Configuration of command-line interface.
CLIMode:2

#  Configuration of heartbeat.
HeartbeatLed:1

#  If this option is set to true, standard reporting is enabled.
EnableStandardReporting:false

#  If the device needs to perform inter-PAN sends, then this option should be
#  enabled.
EnableInterPanSend:false

#  If the device needs to perform inter-PAN receives, then this option should be
#  enabled.
EnableInterPanReceive:false

#  Enable serial commands for ZDO.
EnableZdoSerialCommands:false

#  Enable this option if you wish to enable device bindings.
EnableBindings:true

#  Turn this option on, if end-device binding is enabled.
EnableEndDeviceBind:false

#  Enables the statistics receiving.
EnableReceiveStatistics:false

#  If true, then command discovery commands are supported.
SupportCommandDiscovery:true

#  Selects whether application will use the ECC 163k1 library.
UseEcc163k1:false

#  Selects whether application will use the ECC 283k1 library.
UseEcc283k1:false

#  Enable preconfigured keys for security.
PreconfiguredKeyEnabled:false

#  Enable network key.
NetworkKeyEnabled:false

#  If this option is turned on, then appBuilder will automatically generate the
#  files, immediately upon saving the ISC file.
AutoGenerate:false

#  Enable key switching.
EnableKeySwitch:false

#  Use this setting to turn on fragmentation.
FragmentationEnable:false

#  Enables concentrator support
EnableConcentrator:true

#  If true, then this concentrator is low ram, otherwise high ram
LowRamConcentrator:true

#  If this option is set to true, then MFG_INSTALL_CODE token is used for
#  setting the security install code.
UseSeInstallCodes:false

#  If this option is turned on, then the code will enable the checking of the
#  attributes.
EnableAttributeRangeChecking:false

#  Enable application handling of supported ZigBee Device Object messages.
ReceiveSupportedZdoRequests:false

#  Enable application handling of unsupported ZigBee Device Object messages.
HandleUnsupportedZdoRequests:false

#  Enable application handling of ZigBee Device Object requests related to
#  endpoints.
HandleEndpointZdoRequests:false

#  Enable application handling of ZigBee Device Object requests related to
#  bindings.
HandleBindingZdoRequests:false

#  Use token for TX power mode.
TxPowerModeUseToken:true

#  Enable boost power mode.
BoostMode:false

#  Enable the alternate transmitter output.
AlternatePowerMode:false

#  Use legacy CLI instead of generated CLI.
LegacyCli:false

#  Add Custom CLI sub-menu
AddCustomCli:false

#  Include command and argument descriptions in the embedded code.
IncludeCommandDescriptions:false

#  If set, then project-specific callbacks file will be generated.
GenerateCallbacksFile:false

#  The manufacturer code for this app defaults to 0.
ManufacturerCodeDefaultIsZero:true

#  Actual preconfigured key, if it is enabled.
PreconfiguredKey:56777777777777777777777777777777

#  Actual network key.
NetworkKey:12333333333333333333333333333333

#  Actual second network key.
NetworkKey2:ABCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC


# Setup configurations
{setupId:additionalFiles
}
{setupId:bleGattConfigurator
<?xml version="1.0" encoding="UTF-8"?><gatt generic_attribute_service="false" header="gatt_db.h" name="Custom BLE GATT" out="gatt_db.c" prefix="gattdb_"/>
}
{setupId:boardHeader
allowMissingHeader:false
useHeaderInPlace:false
em357=BOARD,em35x/dev0680,,
efr32~family[M]~series[1]~device_configuration[1]~performance[P]~radio[233]~flash[256K]~temp[G]~package[M]~pins[48]+iar=USE_HARDWARE_CONFIGURATOR,,,
efr32~family[M]~series[1]~device_configuration[1]~performance[P]~radio[233]~flash[256K]~temp[G]~package[M]~pins[48]+BRD4150A+iar=USE_HARDWARE_CONFIGURATOR,,,
efr32~family[M]~series[1]~device_configuration[2]~performance[P]~radio[332]~flash[1024K]~temp[G]~package[L]~pins[125]+BRD4162A+gcc=USE_HARDWARE_CONFIGURATOR,,,
efr32~family[M]~series[1]~device_configuration[2]~performance[P]~radio[332]~flash[1024K]~temp[G]~package[L]~pins[125]+BRD4162A+iar=USE_HARDWARE_CONFIGURATOR,,,
}
{setupId:bookkeeping
}
{setupId:bootloader
}
{setupId:callbackConfiguration
}
{setupId:debugConfiguration
on
area name off
appSerial=1
remove,ATTRIBUTES
compile,CUSTOM1
compile,CUSTOM2
compile,ZDO
disable,CUSTOM2
enable,DEBUG
}
{setupId:halOptions
}
{setupId:hwConfig
featureLevel=1
active=true
}
{setupId:information
\{key:description
Zigbee switch application using NVM3 designed to work with the dynamic
multiprotocol demonstration light

The Dynamic Multiprotocol Demo Switch application helps demonstrate the dynamic
multiprotocol feature from Silabs. This application only uses zigbee and is not
a dynamic multiprotocol application itself. This application is to be used with
the Dynamic Multiprotocol Demo Light sample to demonstrate the control of a 
dynamic multiprotocol device from a zigbee network.

The Demo is set up to run on the WSTK6000B Mesh Development Kit. The Demo makes
use of the LCD display, LEDs, and buttons on the WSTK. 

The Switch is configured to join a zigbee network as a router and once joined it
finds and binds to an on/off server cluster such that, after joining, button 
presses on the WSTK will send the on/off cluster's Toggle command to the bound
device. The Switch will also set up reporting on the bound device to report any
change in state of the on/off cluster. The state of the on/off attribute is then
shown on the LCD display by the bulb icon.

Upon startup, a help screen is shown on the LCD display to assist the user to 
join and leave the network and to control the Light. 

All application code is contained in the _callbacks.c files within each
application directory.

To use each application:

   1. Load the included application configuration file (i.e., the .isc file)
      into Simplicity Studio.

   2. Enter a new name for the application in the pop-up window.

   3. Generate the application's header and project/workspace files by
      clicking on the "Generate" button in Simplicity Studio.  The application
      files will be generated in the app/builder/<name> directory in the stack
      installation location.

   4. Load the generated project file into the appropriate compiler and build
      the project.

   5. Load the binary image onto a device using Simplicity Studio.
\}
}
{setupId:macros
-DDEVICE_TYPE=1
-DNO_LED=1
TRANSITION_TIME_DS=20
-DEMBER_AF_DISCOVERY_TIMEOUT_QS=20
}
{setupId:mpsi
- mappings
- custom messages
}
{setupId:quizz
}
{setupId:rf4ce
nodeCapabilities=0
vendorId=65521
vendorString=
userString=
deviceTypes=[254]
profileIds=[0]
power=3
}
{setupId:rf4ceMso
}
{setupId:rf4ceZrc
}
{setupId:serial
}
{setupId:template
}
{setupId:token
}
#  The name of the set of Command Line Interface (CLI) commands that are
#  compiled into the application by default.
CliCommandSet:Full

#  These are the various Command Line Interface (CLI) commands that can be
#  included, or excluded (if they are included by default), in the application.
CliCommands:compile,plugin green-power-client add-group-sink

CliCommands:compile,plugin green-power-client add-sink

CliCommands:compile,plugin green-power-client clear-proxy-table

CliCommands:compile,plugin green-power-client duplicate-filter-test

CliCommands:compile,plugin green-power-client print-proxy-table

CliCommands:compile,plugin green-power-client rm-gpd

CliCommands:compile,plugin green-power-client rm-sink

CliCommands:compile,plugin green-power-client set-key

CliCommands:compile,plugin green-power-client set-proxy-entry

CliCommands:remove,zcl color-control emovehue

CliCommands:remove,zcl color-control emovetohue

CliCommands:remove,zcl color-control emovetohueandsat

CliCommands:remove,zcl color-control estephue

CliCommands:remove,zcl color-control loop

CliCommands:remove,zcl color-control movecolor

CliCommands:remove,zcl color-control movecolortemp

CliCommands:remove,zcl color-control movehue

CliCommands:remove,zcl color-control movesat

CliCommands:remove,zcl color-control movetocolor

CliCommands:remove,zcl color-control movetocolortemp

CliCommands:remove,zcl color-control movetohue

CliCommands:remove,zcl color-control movetohueandsat

CliCommands:remove,zcl color-control movetosat

CliCommands:remove,zcl color-control stepcolor

CliCommands:remove,zcl color-control stepcolortemp

CliCommands:remove,zcl color-control stephue

CliCommands:remove,zcl color-control stepsat

CliCommands:remove,zcl color-control stopmovestep

CliCommands:remove,zcl scenes add

CliCommands:remove,zcl scenes copy

CliCommands:remove,zcl scenes eadd

CliCommands:remove,zcl scenes eview

CliCommands:remove,zcl scenes get

CliCommands:remove,zcl scenes recall

CliCommands:remove,zcl scenes remove

CliCommands:remove,zcl scenes rmall

CliCommands:remove,zcl scenes store

CliCommands:remove,zcl scenes view

#  Plugin configuration
appPlugin:address-table,false

appPlugin:aes-cmac,false

appPlugin:basic,true

appPlugin:button-joining,false

appPlugin:calendar-client,true

appPlugin:calendar-common,false

appPlugin:calendar-server,true

appPlugin:coexistence,true

appPlugin:color-control,true

appPlugin:color-control-server,false

appPlugin:command-relay,false

appPlugin:comms-hub-function,false

appPlugin:concentrator,false

appPlugin:counters,true

appPlugin:device-database,false

appPlugin:device-management-client,false

appPlugin:device-management-server,false

appPlugin:device-query-service,false

appPlugin:device-table,false

appPlugin:diagnostic-server,true

appPlugin:dmp-ui-demo,true

appPlugin:door-lock-server,true

appPlugin:drlc,true

appPlugin:drlc-server,false

appPlugin:ember-minimal-printf,true

appPlugin:end-device-support,false

appPlugin:esi-management,true

appPlugin:events-client,false

appPlugin:events-server,false

appPlugin:exosite-demo,false

appPlugin:ezmode-commissioning,false

appPlugin:find-and-bind-initiator,true

appPlugin:find-and-bind-target,false

appPlugin:form-and-join,true

appPlugin:fragmentation,false

appPlugin:gas-proxy-function,false

appPlugin:gbcs-device-log,false

appPlugin:gbcs-gas-meter,false

appPlugin:gbz-message-controller,false

appPlugin:general-response-commands,false

appPlugin:green-power-client,true

appPlugin:green-power-common,true

appPlugin:green-power-server,false

appPlugin:green-power-test-device,false

appPlugin:groups-client,true

appPlugin:groups-server,true

appPlugin:hc-11073-tunnel,true

appPlugin:heartbeat,false

appPlugin:ias-zone-client,false

appPlugin:ias-zone-server,false

appPlugin:identify,true

appPlugin:identify-feedback,false

appPlugin:infrared-led,false

appPlugin:interpan,true

appPlugin:key-establishment,true

appPlugin:level-control,true

appPlugin:lwip,false

appPlugin:lwip-callback-tests,false

appPlugin:lwip-interface,false

appPlugin:lwip-stats,false

appPlugin:lwip-udp-wrapper,false

appPlugin:manufacturing-library-cli,false

appPlugin:messaging-client,true

appPlugin:messaging-server,true

appPlugin:meter-mirror,false

appPlugin:meter-snapshot-client,false

appPlugin:meter-snapshot-server,false

appPlugin:meter-snapshot-storage,false

appPlugin:mn-price-passthrough,false

appPlugin:network-creator,false

appPlugin:network-creator-security,false

appPlugin:network-find,false

appPlugin:network-steering,true

appPlugin:on-off,true

appPlugin:ota-bootload,false

appPlugin:ota-client,false

appPlugin:ota-client-policy,false

appPlugin:ota-common,false

appPlugin:ota-server,false

appPlugin:ota-server-policy,false

appPlugin:ota-storage-common,false

appPlugin:ota-storage-posix-filesystem,false

appPlugin:ota-storage-simple,false

appPlugin:ota-storage-simple-eeprom,false

appPlugin:ota-storage-simple-ram,false

appPlugin:partner-link-key-exchange,true

appPlugin:permit-join-manager,false

appPlugin:poll-control-client,true

appPlugin:poll-control-server,true

appPlugin:power-consumption-model,false

appPlugin:prepayment-client,false

appPlugin:prepayment-server,false

appPlugin:prepayment-snapshot-storage,false

appPlugin:price-client,true

appPlugin:price-common,false

appPlugin:price-server,true

appPlugin:reporting,false

appPlugin:scan-dispatch,true

appPlugin:scenes,true

appPlugin:scenes-client,false

appPlugin:simple-clock,false

appPlugin:simple-main,true

appPlugin:simple-metering-client,true

appPlugin:simple-metering-server,true

appPlugin:sleepy-message-queue,false

appPlugin:smart-energy-registration,false

appPlugin:stack-diagnostics,false

appPlugin:standalone-bootloader-client,false

appPlugin:standalone-bootloader-common,false

appPlugin:standalone-bootloader-server,false

appPlugin:standard-printf-support,false

appPlugin:sub-ghz-client,false

appPlugin:sub-ghz-server,false

appPlugin:test-harness,false

appPlugin:test-harness-z3,false

appPlugin:throughput,false

appPlugin:throughput-library,false

appPlugin:time-server,true

appPlugin:trust-center-backup,false

appPlugin:trust-center-keepalive,false

appPlugin:trust-center-nwk-key-update-broadcast,false

appPlugin:trust-center-nwk-key-update-periodic,false

appPlugin:trust-center-nwk-key-update-unicast,false

appPlugin:tunneling-client,true

appPlugin:tunneling-server,true

appPlugin:update-tc-link-key,true

appPlugin:xmodem-sender,false

appPlugin:zcl-ip,false

appPlugin:zll-commissioning,true

appPlugin:zll-identify-server,true

appPlugin:zll-level-control-server,true

appPlugin:zll-on-off-server,true

appPlugin:zll-scenes-client,false

appPlugin:zll-scenes-server,true

appPlugin:zll-utility-client,true

appPlugin:zll-utility-server,false

appPlugin:ble,false

appPlugin:bulb-pwm-cli,false

appPlugin:bulb-ui,false

appPlugin:configuration-server,false

appPlugin:connection-manager,false

appPlugin:electrical-measurement-server,false

appPlugin:em4,false

appPlugin:idle-sleep,true

appPlugin:illuminance-measurement-server,false

appPlugin:led-dim-pwm,false

appPlugin:led-rgb-pwm,false

appPlugin:led-temp-pwm,false

appPlugin:low-voltage-shutdown,false

appPlugin:mac-address-filtering,false

appPlugin:manufacturing-library-ota,false

appPlugin:mbedtls,false

appPlugin:metering-server,false

appPlugin:micrium-rtos,false

appPlugin:occupancy-pyd1698-cli,false

appPlugin:occupancy-sensor-server,false

appPlugin:power-configuration-server,false

appPlugin:relative-humidity-measurement-server,false

appPlugin:security-sensor,false

appPlugin:silabs-device-ui,false

appPlugin:temperature-measurement-server,false

appPlugin:binding-table-library,true

appPlugin:cbke-163k1-library,false

appPlugin:cbke-283k1-library,false

appPlugin:cbke-library-core,false

appPlugin:cbke-library-dsa-sign,false

appPlugin:cbke-library-dsa-verify,false

appPlugin:cbke-library-dsa-verify-283k1,false

appPlugin:debug-basic-library,true

appPlugin:debug-extended-library,false

appPlugin:ecc-library-163k1,false

appPlugin:ecc-library-283k1,false

appPlugin:end-device-bind-library,false

appPlugin:gp-library,true

appPlugin:install-code-library,true

appPlugin:manufacturing-library,false

appPlugin:multi-network-library,false

appPlugin:packet-validate-library,true

appPlugin:security-library-core,true

appPlugin:security-link-keys-library,false

appPlugin:zigbee-pro-bc-table-library,false

appPlugin:zigbee-pro-bc-table-mbedtls-library,false

appPlugin:zigbee-pro-leaf-library,false

appPlugin:zigbee-pro-library,true

appPlugin:zigbee-r22-support-library,false

appPlugin:zll-library,true

appPlugin:debug-jtag,false

appPlugin:debug-jtag-stub,true

appPlugin:hal-library,true

appPlugin:hal-library-rtos,false

appPlugin:humidity-si7021,false

appPlugin:i2c-driver,false

appPlugin:illuminance-si1141,false

appPlugin:psstore,false

appPlugin:serial,true

appPlugin:sim-eeprom1,false

appPlugin:sim-eeprom2,false

appPlugin:sim-eeprom2-1to2-upgrade,false

appPlugin:sim-eeprom2-1to2-upgrade-stub,false

appPlugin:sim-eeprom2-to-nvm3-upgrade,false

appPlugin:sim-eeprom2-to-nvm3-upgrade-stub,true

appPlugin:temperature-si7021,false

appPlugin:temperature-si7021-stub,false

appPlugin:temperature-si7053,false

appPlugin:wstk-display,true

appPlugin:adc,true

appPlugin:antenna,false

appPlugin:antenna-stub,true

appPlugin:extdev,false

appPlugin:ezradiopro,false

appPlugin:fem-control,false

appPlugin:glib,true

appPlugin:humidity-si7021-stub,false

appPlugin:i2c-driver-stub,false

appPlugin:illuminance-si1141-stub,false

appPlugin:pa,true

appPlugin:pti,true

appPlugin:temperature-si7053-stub,false

appPlugin:rail-library,true

appPlugin:rail-library-mp,false

appPlugin:mpsi,false

appPlugin:battery-monitor,false

appPlugin:battery-monitor-stub,false

appPlugin:bulb-pwm-driver,false

appPlugin:button-interface,false

appPlugin:button-interface-stub,false

appPlugin:eeprom,true

appPlugin:generic-interrupt-control,false

appPlugin:generic-interrupt-control-stub,false

appPlugin:gpio-sensor,false

appPlugin:gpio-sensor-stub,false

appPlugin:led-blink,false

appPlugin:led-blink-stub,false

appPlugin:occupancy-pyd1698,false

appPlugin:occupancy-pyd1698-stub,false

appPlugin:power-meter-cs5463,false

appPlugin:power-meter-cs5463-stub,false

appPlugin:sb1-gesture-sensor,false

appPlugin:sb1-gesture-sensor-stub,false

appPlugin:tamper-switch,false

appPlugin:tamper-switch-stub,false

appPlugin:linked-list,false

appPlugin:module-lna,false

appPlugin:mpsi-ipc,false

appPlugin:mpsi-storage,false

appPlugin:transport-mqtt,false

appPlugin:slot-manager,false

appPlugin:cjson,false

appPlugin:libcoap,false

appPlugin:paho.mqtt.c,false

appPlugin:nvm3,true

#  Plugin specific options
AppPluginOption:EMBER_AF_PLUGIN_NETWORK_COMMISSIONER_TOUCHLINK_COMMISSIONING,TRUE

AppPluginOption:EMBER_AF_PLUGIN_NETWORK_COMMISSIONER_NETWORK_FORMATION,FALSE

AppPluginOption:EMBER_BINDING_TABLE_SIZE,10

AppPluginOption:EMBER_AF_PLUGIN_END_DEVICE_SUPPORT_ENHANCED_SLEEP_SUPPORT,TRUE

AppPluginOption:EMBER_AF_PLUGIN_FIND_AND_BIND_INITIATOR_TARGET_RESPONSES_DELAY_MS,8000