# Auto-generated file, Do not modify!
# Generated by sample-apps-regenerate.pl

DynamicMultiprotocolDemoLight {
  name=DynamicMultiprotocolDemoLight 
  dir=multiprotocol/DynamicMultiprotocolDemoLight
  isc=multiprotocol/DynamicMultiprotocolDemoLight/DynamicMultiprotocolDemoLightSoc.isc
  include=DynamicMultiprotocolDemoLight_callbacks.c, .internal_hwconfig
  demo.1.bin=multiprotocol/DynamicMultiprotocolDemoLight/efr32mg12p432f1024gl125-brd4161a/DynamicMultiprotocolDemoLight.s37
  demo.1.arch=efr32mg12p432f1024gl125+brd4161a
  demo.2.bin=multiprotocol/DynamicMultiprotocolDemoLight/efr32mg12p332f1024gl125-brd4162a/DynamicMultiprotocolDemoLight.s37
  demo.2.arch=efr32mg12p332f1024gl125+brd4162a
  architecture=BRD4161A+iar, BRD4165B+iar, BRD4162A+iar
  This is a sample application demonstrating a light application using dynamic multiprotocol (ZigBee + BLE). Requires IAR.
}

DynamicMultiprotocolDemoLightSed {
  name=DynamicMultiprotocolDemoLightSed 
  dir=multiprotocol/DynamicMultiprotocolDemoLightSed
  isc=multiprotocol/DynamicMultiprotocolDemoLightSed/DynamicMultiprotocolDemoLightSedSoc.isc
  include=DynamicMultiprotocolDemoLightSed_callbacks.c, .internal_hwconfig
  demo.1.bin=multiprotocol/DynamicMultiprotocolDemoLightSed/efr32mg12p432f1024gl125-brd4161a/DynamicMultiprotocolDemoLightSed.s37
  demo.1.arch=efr32mg12p432f1024gl125+brd4161a
  demo.2.bin=multiprotocol/DynamicMultiprotocolDemoLightSed/efr32mg12p332f1024gl125-brd4162a/DynamicMultiprotocolDemoLightSed.s37
  demo.2.arch=efr32mg12p332f1024gl125+brd4162a
  architecture=BRD4161A+iar, BRD4165B+iar, BRD4162A+iar
  This is a sample application demonstrating a sleepy light application using dynamic multiprotocol (ZigBee + BLE). Requires IAR.
}

DynamicMultiprotocolDemoLightSedWithNvm3 {
  name=DynamicMultiprotocolDemoLightSedWithNvm3 
  dir=multiprotocol/DynamicMultiprotocolDemoLightSedWithNvm3
  isc=multiprotocol/DynamicMultiprotocolDemoLightSedWithNvm3/DynamicMultiprotocolDemoLightSedWithNvm3Soc.isc
  include=DynamicMultiprotocolDemoLightSedWithNvm3_callbacks.c, .internal_hwconfig
  This is a sample application demonstrating a sleepy light application using dynamic multiprotocol (ZigBee + BLE) and NVM3 for persistent storage. Requires IAR.
}

DynamicMultiprotocolDemoLightWithNvm3 {
  name=DynamicMultiprotocolDemoLightWithNvm3 
  dir=multiprotocol/DynamicMultiprotocolDemoLightWithNvm3
  isc=multiprotocol/DynamicMultiprotocolDemoLightWithNvm3/DynamicMultiprotocolDemoLightWithNvm3Soc.isc
  include=DynamicMultiprotocolDemoLightWithNvm3_callbacks.c, .internal_hwconfig
  This is a sample application demonstrating a light application using dynamic multiprotocol (ZigBee + BLE) and NVM3 for persistent storage. Requires IAR.
}

DynamicMultiprotocolDemoLightWithNvm3_BRD4171A {
  name=DynamicMultiprotocolDemoLightWithNvm3_BRD4171A 
  dir=multiprotocol/DynamicMultiprotocolDemoLightWithNvm3_BRD4171A
  isc=multiprotocol/DynamicMultiprotocolDemoLightWithNvm3_BRD4171A/DynamicMultiprotocolDemoLightWithNvm3Soc_BRD4171A.isc
  include=DynamicMultiprotocolDemoLightWithNvm3_BRD4171A_callbacks.c, .internal_hwconfig
  This is a sample application for BRD4171A demonstrating a light application using dynamic multiprotocol (ZigBee + BLE) and NVM3 for persistent storage. Requires IAR.
}

DynamicMultiprotocolDemoSwitch {
  name=DynamicMultiprotocolDemoSwitch 
  dir=multiprotocol/DynamicMultiprotocolDemoSwitch
  isc=multiprotocol/DynamicMultiprotocolDemoSwitch/DynamicMultiprotocolDemoSwitchSoc.isc
  include=DynamicMultiprotocolDemoSwitch_callbacks.c, .internal_hwconfig
  demo.1.bin=multiprotocol/DynamicMultiprotocolDemoSwitch/efr32mg12p432f1024gl125-brd4161a/DynamicMultiprotocolDemoSwitch.s37
  demo.1.arch=efr32mg12p432f1024gl125+brd4161a
  demo.2.bin=multiprotocol/DynamicMultiprotocolDemoSwitch/efr32mg12p332f1024gl125-brd4162a/DynamicMultiprotocolDemoSwitch.s37
  demo.2.arch=efr32mg12p332f1024gl125+brd4162a
  architecture=BRD4161A+iar, BRD4165B+iar, BRD4162A+iar
  This is a Zigbee switch application designed to work with the dynamic multiprotocol demonstration light. Requires IAR.
}

DynamicMultiprotocolDemoSwitchWithNvm3 {
  name=DynamicMultiprotocolDemoSwitchWithNvm3 
  dir=multiprotocol/DynamicMultiprotocolDemoSwitchWithNvm3
  isc=multiprotocol/DynamicMultiprotocolDemoSwitchWithNvm3/DynamicMultiprotocolDemoSwitchWithNvm3Soc.isc
  include=DynamicMultiprotocolDemoSwitchWithNvm3_callbacks.c, .internal_hwconfig
  This is a Zigbee switch application using NVM3 designed to work with the dynamic multiprotocol demonstration light. Requires IAR.
}

DynamicMultiprotocolDemoSwitchWithNvm3_BRD4171A {
  name=DynamicMultiprotocolDemoSwitchWithNvm3_BRD4171A 
  dir=multiprotocol/DynamicMultiprotocolDemoSwitchWithNvm3_BRD4171A
  isc=multiprotocol/DynamicMultiprotocolDemoSwitchWithNvm3_BRD4171A/DynamicMultiprotocolDemoSwitchWithNvm3Soc_BRD4171A.isc
  include=DynamicMultiprotocolDemoSwitchWithNvm3_BRD4171A_callbacks.c, .internal_hwconfig
  This is a Zigbee switch application for BRD4171A using NVM3 designed to work with the dynamic multiprotocol demonstration light. Requires IAR.
}

DynamicMultiprotocolZigBeeZllLightBle {
  name=DynamicMultiprotocolZigBeeZllLightBle 
  dir=multiprotocol/DynamicMultiprotocolZigBeeZllLightBle
  isc=multiprotocol/DynamicMultiprotocolZigBeeZllLightBle/DynamicMultiprotocolZigBeeZllLightBleSoc.isc
  include=DynamicMultiprotocolZigBeeZllLightBle_callbacks.c, .internal_hwconfig
  architecture=iar
  This is a sample application demonstrating dynamic multiprotocol (ZigBee + BLE). Requires IAR.
}

SwitchedMultiprotocolJoiningDevice {
  name=SwitchedMultiprotocolJoiningDevice 
  dir=multiprotocol/SwitchedMultiprotocolJoiningDevice
  isc=multiprotocol/SwitchedMultiprotocolJoiningDevice/SwitchedMultiprotocolJoiningDeviceSoc.isc
  include=SwitchedMultiprotocolJoiningDevice_callbacks.c, .internal_hwconfig
  This is a sample application demonstrating switched multiprotocol, acting as a joining device. This application uses zigbee 3.0 security. Requires IAR.
}

Z3CapSenseDimmerSwitch {
  name=Z3CapSenseDimmerSwitch 
  dir=z3/Z3CapSenseDimmerSwitch
  isc=z3/Z3CapSenseDimmerSwitch/Z3CapSenseDimmerSwitchSoc.isc
  include=Z3CapSenseDimmerSwitch_callbacks.c
  This is a Zigbee 3.0 sensor application.  The application provides open/close state of a magnetic reed switch and device tamper detection.  It is intended to be used with the Z3Gateway, available as a sample application, or with the Zigbee gateway reference designs RD-0001-0201 and RD-0002-0201.  Use the application with kit RD-0039-0201 (EM3587).
}

Z3ColorControlLight {
  name=Z3ColorControlLight 
  dir=z3/Z3ColorControlLight
  isc=z3/Z3ColorControlLight/Z3ColorControlLightSoc.isc
  include=Z3ColorControlLight_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 light application.  The application provides pwm control for dimming, and pwm mixing for color functions.  It is intended to be used with the Z3Gateway sample application, or with the Zigbee gateway reference designs RD-0001-0201 and RD-0002-0201.  Use the application with kits RD-0035-0601 (EM3585), RD-0085-0401 (EFR32MG1P732F256IM32) and RD-0098-0401 (EFR32MG12P432F1024IM32).
}

Z3ColorTempLight {
  name=Z3ColorTempLight 
  dir=z3/Z3ColorTempLight
  isc=z3/Z3ColorTempLight/Z3ColorTempLightSoc.isc
  include=Z3ColorTempLight_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 light application.  The application provides pwm control for dimming, and pwm mixing for color temperature functions.  It is intended to be used with the Z3Gateway sample application, or with the Zigbee gateway reference designs RD-0001-0201 and RD-0002-0201.  Use the application with kits RD-0035-0601 (EM3585), RD-0085-0401 (EFR32MG1P732F256IM32) and RD-0098-0401 (EFR32MG12P432F1024IM32).
}

Z3ContactSensor {
  name=Z3ContactSensor 
  dir=z3/Z3ContactSensor
  isc=z3/Z3ContactSensor/Z3ContactSensorSoc.isc
  include=Z3ContactSensor_callbacks.c
  This is a Zigbee 3.0 sensor application.  The application provides open/close state of a magnetic reed switch and device tamper detection.  It is intended to be used with the Z3Gateway, available as a sample application, or with the Zigbee gateway reference designs RD-0001-0201 and RD-0002-0201.  Use the application with kit RD-0030-0201 (EM3587).
}

Z3ContactSensorWithWwah {
  name=Z3ContactSensorWithWwah 
  dir=z3/Z3ContactSensorWithWwah
  isc=z3/Z3ContactSensorWithWwah/Z3ContactSensorWithWwahSoc.isc
  include=Z3ContactSensorWithWwah_callbacks.c
  This is the Zigbee 3.0 contact sensor application with the Works With All Hubs cluster enabled.
}

Z3DimmableLight {
  name=Z3DimmableLight 
  dir=z3/Z3DimmableLight
  isc=z3/Z3DimmableLight/Z3DimmableLightSoc.isc
  include=Z3DimmableLight_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 light application.  The application provides pwm control for a dimming function.  It is intended to be used with the Z3Gateway sample application, or with the Zigbee gateway reference designs RD-0001-0201 and RD-0002-0201.  Use the application with kits RD-0035-0601 (EM3585), RD-0085-0401 (EFR32MG1P732F256IM32), RD-0098-0401 (EFR32MG12P432F1024IM32), WSTK (EFR32) and EM35X-DEV (EM358x).
}

Z3DoorLockWithWwah {
  name=Z3DoorLockWithWwah 
  dir=z3/Z3DoorLockWithWwah
  isc=z3/Z3DoorLockWithWwah/Z3DoorLockWithWwahSoc.isc
  include=Z3DoorLockWithWwah_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 end device door-lock application with the Works With All Hubs cluster enabled.
}

Z3Light {
  name=Z3Light 
  dir=z3/Z3Light
  isc=z3/Z3Light/Z3LightSoc.isc
  include=Z3Light_callbacks.c, .internal_hwconfig
  demo.1.bin=z3/Z3Light/efr32mg1p232f256gm48/Z3Light.s37
  demo.1.arch=efr32mg1p232f256gm48+brd4151a
  demo.2.bin=z3/Z3Light/efr32mg1p132f256gm48/Z3Light.s37
  demo.2.arch=efr32mg1p132f256gm48+brd4153a
  demo.3.bin=z3/Z3Light/efr32mg12p432f1024gl125-brd4161a/Z3Light.s37
  demo.3.arch=efr32mg12p432f1024gl125+brd4161a
  demo.4.bin=z3/Z3Light/efr32mg12p332f1024gl125-brd4162a/Z3Light.s37
  demo.4.arch=efr32mg12p332f1024gl125+brd4162a
  This is a ZigBee 3.0 light application.
}

Z3LightCombo {
  name=Z3LightCombo 
  dir=z3/Z3LightCombo
  isc=z3/Z3LightCombo/Z3LightComboSoc.isc
  include=Z3LightCombo_callbacks.c, .internal_hwconfig
  This is a ZigBee 3.0 light application with Green Power Combo Basic functionality.
}

Z3LightWithNvm3 {
  name=Z3LightWithNvm3 
  dir=z3/Z3LightWithNvm3
  isc=z3/Z3LightWithNvm3/Z3LightWithNvm3Soc.isc
  include=Z3LightWithNvm3_callbacks.c, .internal_hwconfig
  This is a ZigBee 3.0 light application using NVM3 as the persistent storage
}

Z3LightWithWwah {
  name=Z3LightWithWwah 
  dir=z3/Z3LightWithWwah
  isc=z3/Z3LightWithWwah/Z3LightWithWwahSoc.isc
  include=Z3LightWithWwah_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 router light application with the Works With All Hubs cluster enabled.
}

Z3Light_BRD4176A {
  name=Z3Light_BRD4176A 
  dir=z3/Z3Light_BRD4176A
  isc=z3/Z3Light_BRD4176A/Z3LightSoc_BRD4176A.isc
  include=Z3Light_BRD4176A_callbacks.c, .internal_hwconfig
  demo.1.bin=z3/Z3Light_BRD4176A/efr32mg21a010f1024im32/Z3Light_BRD4176A.s37
  demo.1.arch=efr32mg21a010f1024im32+brd4176a
  
  This is a ZigBee 3.0 light application for BRD4176A.
}

Z3OccupancySensor {
  name=Z3OccupancySensor 
  dir=z3/Z3OccupancySensor
  isc=z3/Z3OccupancySensor/Z3OccupancySensorSoc.isc
  include=Z3OccupancySensor_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 sensor application.  The application provides occupancy sensing, temperature measurement, relative humidity measurement, and illuminance measurement.  It is intended to be used with the Z3Gateway sample application, or with the Zigbee gateway reference designs RD-0001-0201 and RD-0002-0201.  Use the application with kits RD-0078-0201 (EFR32MG1P232F256GM48) and RD-0099-0201 (EFR32MG12P432F1024GM48).
}

Z3SleepyDoorLockWithWwah {
  name=Z3SleepyDoorLockWithWwah 
  dir=z3/Z3SleepyDoorLockWithWwah
  isc=z3/Z3SleepyDoorLockWithWwah/Z3SleepyDoorLockWithWwahSoc.isc
  include=Z3SleepyDoorLockWithWwah_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 sleepy end device door-lock application with the Works With All Hubs cluster enabled.
}

Z3SmartOutlet {
  name=Z3SmartOutlet 
  dir=z3/Z3SmartOutlet
  isc=z3/Z3SmartOutlet/Z3SmartOutletSoc.isc
  include=Z3SmartOutlet_callbacks.c, .internal_hwconfig
  This is a Zigbee 3.0 sensor and actuator application.  The application provides outlet on/off control; over-current and over-temperature shutdown; and power, temperature, relative humidity and illuminance measurements.    It is intended to be used with the Z3Gateway sample application, or with the Zigbee gateway reference designs RD-0001-0201 and RD-0002-0201.  Use the application with kits RD-0051-0201 (EFR32MG1P232F256GM48) and RD-0100-0201 (EFR32MG12P432F1024GM48).
}

Z3Switch {
  name=Z3Switch 
  dir=z3/Z3Switch
  isc=z3/Z3Switch/Z3SwitchSoc.isc
  include=Z3Switch_callbacks.c, .internal_hwconfig
  demo.1.bin=z3/Z3Switch/efr32mg1p232f256gm48/Z3Switch.s37
  demo.1.arch=efr32mg1p232f256gm48+brd4151a
  demo.2.bin=z3/Z3Switch/efr32mg1p132f256gm48/Z3Switch.s37
  demo.2.arch=efr32mg1p132f256gm48+brd4153a
  demo.3.bin=z3/Z3Switch/efr32mg12p432f1024gl125-brd4161a/Z3Switch.s37
  demo.3.arch=efr32mg12p432f1024gl125+brd4161a
  demo.4.bin=z3/Z3Switch/efr32mg12p332f1024gl125-brd4162a/Z3Switch.s37
  demo.4.arch=efr32mg12p332f1024gl125+brd4162a
  This is a ZigBee 3.0 switch application.
}

Z3SwitchWithMicrium {
  name=Z3SwitchWithMicrium 
  dir=z3/Z3SwitchWithMicrium
  isc=z3/Z3SwitchWithMicrium/Z3SwitchWithMicriumSoc.isc
  include=Z3SwitchWithMicrium_callbacks.c, .internal_hwconfig
  architecture=iar
  This is a ZigBee 3.0 switch application, with Micrium.
}

Z3SwitchWithNvm3 {
  name=Z3SwitchWithNvm3 
  dir=z3/Z3SwitchWithNvm3
  isc=z3/Z3SwitchWithNvm3/Z3SwitchWithNvm3Soc.isc
  include=Z3SwitchWithNvm3_callbacks.c, .internal_hwconfig
  This is a ZigBee 3.0 switch application using NVM3 as the persistent storage
}

Z3Switch_BRD4176A {
  name=Z3Switch_BRD4176A 
  dir=z3/Z3Switch_BRD4176A
  isc=z3/Z3Switch_BRD4176A/Z3SwitchSoc_BRD4176A.isc
  include=Z3Switch_BRD4176A_callbacks.c, .internal_hwconfig
  demo.1.bin=z3/Z3Switch_BRD4176A/efr32mg21a010f1024im32/Z3Switch_BRD4176A.s37
  demo.1.arch=efr32mg21a010f1024im32+brd4176a
  
  This is a ZigBee 3.0 switch application for BRD4176A.
}

HaSampleGateway {
  name=HaSampleGateway 
  dir=zha/HaSampleGateway
  isc=zha/HaSampleGateway/HaSampleGatewaySoc.isc
  include=HaSampleGateway_callbacks.c, .internal_hwconfig
  This is a gateway application for a Home Automation Network.
}

HaSampleLight {
  name=HaSampleLight 
  dir=zha/HaSampleLight
  isc=zha/HaSampleLight/HaSampleLightSoc.isc
  include=HaSampleLight_callbacks.c, .internal_hwconfig
  This is an on/off light for a Home Automation network.
}

HaSampleSwitch {
  name=HaSampleSwitch 
  dir=zha/HaSampleSwitch
  isc=zha/HaSampleSwitch/HaSampleSwitchSoc.isc
  include=HaSampleSwitch_callbacks.c, .internal_hwconfig
  This is a switch application for a Home Automation Network.
}

ZllSampleController {
  name=ZllSampleController 
  dir=zll/ZllSampleController
  isc=zll/ZllSampleController/ZllSampleControllerSoc.isc
  include=ZllSampleController_callbacks.c, .internal_hwconfig
  This is a controller application for a ZLL network.
}

ZllSampleLight {
  name=ZllSampleLight 
  dir=zll/ZllSampleLight
  isc=zll/ZllSampleLight/ZllSampleLightSoc.isc
  include=ZllSampleLight_callbacks.c, .internal_hwconfig
  This is a simple on/off light application for a ZLL network.
}

SeSample12bIhd {
  name=SeSample12bIhd 
  dir=zse/SeSample12bIhd
  isc=zse/SeSample12bIhd/SeSample12bIhdSoc.isc
  include=SeSample12bIhd_callbacks.c, .internal_hwconfig
  This is an In-Home Display application for a Smart Energy 1.2b network. NOTE: Appropriate CBKE and ECC libraries MUST be enabled or this application will not build.
}

SeSampleEsi {
  name=SeSampleEsi 
  dir=zse/SeSampleEsi
  isc=zse/SeSampleEsi/SeSampleEsiSoc.isc
  include=SeSampleEsi_callbacks.c, .internal_hwconfig
  This is an Energy Services Interface application for a Smart Energy 1.x network. NOTE: Appropriate CBKE and ECC libraries MUST be enabled or this application will not build.
}

SeSampleGSME {
  name=SeSampleGSME 
  dir=zse/SeSampleGSME
  isc=zse/SeSampleGSME/SeSampleGSMESoc.isc
  include=SeSampleGSME_callbacks.c, .internal_hwconfig
  This is a gas meter application for a Smart Energy 1.x network. NOTE: Appropriate CBKE and ECC libraries MUST be enabled or this application will not build.
}

SeSamplePCT {
  name=SeSamplePCT 
  dir=zse/SeSamplePCT
  isc=zse/SeSamplePCT/SeSamplePCTSoc.isc
  include=SeSamplePCT_callbacks.c, .internal_hwconfig
  This is a Programmable Communicating Thermostat application for a Smart Energy 1.x network. NOTE: Appropriate CBKE and ECC libraries MUST be enabled or this application will not build.
}

