#ISD App Configuration:3.1
# ISD version: 4.21.0.201709202024-1504
#  Identified of a stack descriptor used for this configuration. This should not
#  be changed manually, unless you really know what you are doing.
ConfiguratorID:auto-EM35X

#  Output directory which is used as a root for all generated files. The actual
#  files relative to that directory are defined by individual file name.
GenerationDirectory:__SAMPLE_APPLICATION__

#  Unique identifier for this device. This string should be in a form of a C
#  identifier, as it will be used in both generated variable, macros, as well as
#  file names. You should generally not use characters which are not valid
#  characters in a C identifier here.
DeviceName:DynamicMultiprotocolDemoLightSed

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Primary,-1

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Primary,zcustom

#  Overrides a particular client configuration. This happens when you have
#  chosen to include/exclude a client cluster that is optional. Contains
#  'clusterId', 'exclude/include' and the endpoint type name.
OverrideClient:0,exclude,Primary

OverrideClient:1,exclude,Primary

OverrideClient:2,exclude,Primary

OverrideClient:3,exclude,Primary

OverrideClient:4,exclude,Primary

OverrideClient:5,exclude,Primary

OverrideClient:6,exclude,Primary

OverrideClient:7,exclude,Primary

OverrideClient:8,exclude,Primary

OverrideClient:9,exclude,Primary

OverrideClient:a,exclude,Primary

OverrideClient:b,exclude,Primary

OverrideClient:f,exclude,Primary

OverrideClient:15,exclude,Primary

OverrideClient:16,exclude,Primary

OverrideClient:19,exclude,Primary

OverrideClient:1a,exclude,Primary

OverrideClient:1b,exclude,Primary

OverrideClient:20,exclude,Primary

OverrideClient:21,exclude,Primary

OverrideClient:25,exclude,Primary

OverrideClient:100,exclude,Primary

OverrideClient:101,exclude,Primary

OverrideClient:102,exclude,Primary

OverrideClient:103,exclude,Primary

OverrideClient:200,exclude,Primary

OverrideClient:201,exclude,Primary

OverrideClient:202,exclude,Primary

OverrideClient:203,exclude,Primary

OverrideClient:204,exclude,Primary

OverrideClient:300,exclude,Primary

OverrideClient:301,exclude,Primary

OverrideClient:400,exclude,Primary

OverrideClient:401,exclude,Primary

OverrideClient:402,exclude,Primary

OverrideClient:403,exclude,Primary

OverrideClient:404,exclude,Primary

OverrideClient:405,exclude,Primary

OverrideClient:406,exclude,Primary

OverrideClient:40c,exclude,Primary

OverrideClient:40d,exclude,Primary

OverrideClient:40e,exclude,Primary

OverrideClient:40f,exclude,Primary

OverrideClient:410,exclude,Primary

OverrideClient:411,exclude,Primary

OverrideClient:412,exclude,Primary

OverrideClient:413,exclude,Primary

OverrideClient:414,exclude,Primary

OverrideClient:415,exclude,Primary

OverrideClient:416,exclude,Primary

OverrideClient:417,exclude,Primary

OverrideClient:418,exclude,Primary

OverrideClient:419,exclude,Primary

OverrideClient:41a,exclude,Primary

OverrideClient:41b,exclude,Primary

OverrideClient:41c,exclude,Primary

OverrideClient:41d,exclude,Primary

OverrideClient:41e,exclude,Primary

OverrideClient:41f,exclude,Primary

OverrideClient:420,exclude,Primary

OverrideClient:421,exclude,Primary

OverrideClient:422,exclude,Primary

OverrideClient:423,exclude,Primary

OverrideClient:424,exclude,Primary

OverrideClient:425,exclude,Primary

OverrideClient:426,exclude,Primary

OverrideClient:427,exclude,Primary

OverrideClient:428,exclude,Primary

OverrideClient:429,exclude,Primary

OverrideClient:500,exclude,Primary

OverrideClient:501,exclude,Primary

OverrideClient:502,exclude,Primary

OverrideClient:600,exclude,Primary

OverrideClient:601,exclude,Primary

OverrideClient:614,exclude,Primary

OverrideClient:615,exclude,Primary

OverrideClient:700,exclude,Primary

OverrideClient:701,exclude,Primary

OverrideClient:702,exclude,Primary

OverrideClient:703,exclude,Primary

OverrideClient:704,exclude,Primary

OverrideClient:705,exclude,Primary

OverrideClient:706,exclude,Primary

OverrideClient:707,exclude,Primary

OverrideClient:708,exclude,Primary

OverrideClient:709,exclude,Primary

OverrideClient:70a,exclude,Primary

OverrideClient:70b,exclude,Primary

OverrideClient:800,exclude,Primary

OverrideClient:900,exclude,Primary

OverrideClient:901,exclude,Primary

OverrideClient:902,exclude,Primary

OverrideClient:903,exclude,Primary

OverrideClient:904,exclude,Primary

OverrideClient:905,exclude,Primary

OverrideClient:a01,exclude,Primary

OverrideClient:a02,exclude,Primary

OverrideClient:b00,exclude,Primary

OverrideClient:b01,exclude,Primary

OverrideClient:b02,exclude,Primary

OverrideClient:b03,exclude,Primary

OverrideClient:b04,exclude,Primary

OverrideClient:b05,exclude,Primary

OverrideClient:1000,include,Primary

OverrideClient:fc00,exclude,Primary

OverrideClient:fc01,exclude,Primary

OverrideClient:fc02,exclude,Primary

#  Overrides a particular server configuration. This happens when you have
#  chosen to include/exclude a server cluster that is optional. Contains
#  'clusterId', 'exclude/include' and the endpoint type name.
OverrideServer:0,include,Primary

OverrideServer:1,exclude,Primary

OverrideServer:2,exclude,Primary

OverrideServer:3,include,Primary

OverrideServer:4,include,Primary

OverrideServer:5,include,Primary

OverrideServer:6,include,Primary

OverrideServer:7,exclude,Primary

OverrideServer:8,exclude,Primary

OverrideServer:9,exclude,Primary

OverrideServer:a,exclude,Primary

OverrideServer:b,exclude,Primary

OverrideServer:f,exclude,Primary

OverrideServer:15,exclude,Primary

OverrideServer:16,exclude,Primary

OverrideServer:19,exclude,Primary

OverrideServer:1a,exclude,Primary

OverrideServer:1b,exclude,Primary

OverrideServer:20,exclude,Primary

OverrideServer:21,exclude,Primary

OverrideServer:25,exclude,Primary

OverrideServer:100,exclude,Primary

OverrideServer:101,exclude,Primary

OverrideServer:102,exclude,Primary

OverrideServer:103,exclude,Primary

OverrideServer:200,exclude,Primary

OverrideServer:201,exclude,Primary

OverrideServer:202,exclude,Primary

OverrideServer:203,exclude,Primary

OverrideServer:204,exclude,Primary

OverrideServer:300,exclude,Primary

OverrideServer:301,exclude,Primary

OverrideServer:400,exclude,Primary

OverrideServer:401,exclude,Primary

OverrideServer:402,exclude,Primary

OverrideServer:403,exclude,Primary

OverrideServer:404,exclude,Primary

OverrideServer:405,exclude,Primary

OverrideServer:406,exclude,Primary

OverrideServer:40c,exclude,Primary

OverrideServer:40d,exclude,Primary

OverrideServer:40e,exclude,Primary

OverrideServer:40f,exclude,Primary

OverrideServer:410,exclude,Primary

OverrideServer:411,exclude,Primary

OverrideServer:412,exclude,Primary

OverrideServer:413,exclude,Primary

OverrideServer:414,exclude,Primary

OverrideServer:415,exclude,Primary

OverrideServer:416,exclude,Primary

OverrideServer:417,exclude,Primary

OverrideServer:418,exclude,Primary

OverrideServer:419,exclude,Primary

OverrideServer:41a,exclude,Primary

OverrideServer:41b,exclude,Primary

OverrideServer:41c,exclude,Primary

OverrideServer:41d,exclude,Primary

OverrideServer:41e,exclude,Primary

OverrideServer:41f,exclude,Primary

OverrideServer:420,exclude,Primary

OverrideServer:421,exclude,Primary

OverrideServer:422,exclude,Primary

OverrideServer:423,exclude,Primary

OverrideServer:424,exclude,Primary

OverrideServer:425,exclude,Primary

OverrideServer:426,exclude,Primary

OverrideServer:427,exclude,Primary

OverrideServer:428,exclude,Primary

OverrideServer:429,exclude,Primary

OverrideServer:500,exclude,Primary

OverrideServer:501,exclude,Primary

OverrideServer:502,exclude,Primary

OverrideServer:600,exclude,Primary

OverrideServer:601,exclude,Primary

OverrideServer:614,exclude,Primary

OverrideServer:615,exclude,Primary

OverrideServer:700,exclude,Primary

OverrideServer:701,exclude,Primary

OverrideServer:702,exclude,Primary

OverrideServer:703,exclude,Primary

OverrideServer:704,exclude,Primary

OverrideServer:705,exclude,Primary

OverrideServer:706,exclude,Primary

OverrideServer:707,exclude,Primary

OverrideServer:708,exclude,Primary

OverrideServer:709,exclude,Primary

OverrideServer:70a,exclude,Primary

OverrideServer:70b,exclude,Primary

OverrideServer:800,exclude,Primary

OverrideServer:900,exclude,Primary

OverrideServer:901,exclude,Primary

OverrideServer:902,exclude,Primary

OverrideServer:903,exclude,Primary

OverrideServer:904,exclude,Primary

OverrideServer:905,exclude,Primary

OverrideServer:a01,exclude,Primary

OverrideServer:a02,exclude,Primary

OverrideServer:b00,exclude,Primary

OverrideServer:b01,exclude,Primary

OverrideServer:b02,exclude,Primary

OverrideServer:b03,exclude,Primary

OverrideServer:b04,exclude,Primary

OverrideServer:b05,exclude,Primary

OverrideServer:1000,include,Primary

OverrideServer:fc00,exclude,Primary

OverrideServer:fc01,exclude,Primary

OverrideServer:fc02,exclude,Primary

#  Type of the endpoint. Each endpoint implement one endpoint type. There can be
#  one or more endpoint types, regardless of number of actual endpoints.
EndpointType:Green Power,97

#  The ZCL device that this particular endpoint is implementing.
DeviceType:Green Power,GP-proxy-basic

#  ZigBee PRO network configuration.  Each endpoint belongs to a single network
#  configuration.  There can be one or more network configurations.
ZigbeeProNetwork:*Primary,ZA_SLEEPY_END_DEVICE,Z3

#  A list of optional attributes that are included in this configuration. Format
#  is a list of "clusterId,attributeId,<server|client>,manufacturerCode"
#  entries, separated by semicolon.
OptionalAttributes:0,1,server,0:0,5,server,0

#  Attributes that support min/max setting.
BoundAttributes:0,7,server,0:0,3,server,0:0,2,server,0:0,1,server,0:0,0,server,0:3,0,server,0:4,0,server,0:5,4,server,0:5,3,server,0:5,2,server,0:5,1,server,0:5,0,server,0:6,16386,server,0:6,16385,server,0:6,16384,server,0:6,0,server,0

#  Lists the channels that this application will be configured to use.
Channels:11

#  Definitions of individual endpoints. For each endpoint the endpoint number
#  (1-254) is listed, as well as the endpoint type that this endpoint will
#  serve.
ConfiguredEndpoints:*1&260&256&2&Primary&Primary,242&260&256&2&Green Power&Primary

#  A single specification version for each profile defining the max version of
#  the spec supported by this configuration.
SpecVersions:

#  In case of a network coprocessor, this lists a host processor used.
Host:unknown

#  Ember network processor targeted for this application.
Platform:efr32~family[M]~series[1]~device_configuration[2]~performance[P]~radio[332]~flash[1024K]~temp[G]~package[L]~pins[125]+BRD4162A+iar

#  Enable callbacks.
Callbacks:emberAfStackStatusCallback,emberAfMainInitCallback,emberAfPluginOnOffClusterServerPostInitCallback,emberAfOnOffClusterServerAttributeChangedCallback,emberAfPluginBleEventCallback,emberAfPluginBleGetConfigCallback,emberAfMessageSentCallback,emberAfPreCommandReceivedCallback,emberAfPreMessageReceivedCallback,emberAfPreMessageSendCallback,emberAfPreZDOMessageReceivedCallback,emberAfTrustCenterJoinCallback,emberAfHalButtonIsrCallback,emberAfPluginIdleSleepOkToSleepCallback,emberAfPluginIdentifyStopFeedbackCallback,emberAfPluginIdentifyStartFeedbackCallback,emberAfPluginNetworkSteeringCompleteCallback,

#  Any customer-specific general purpose custom events.
CustomEvents:bleEventControl,bleEventHandler

CustomEvents:bleTxEventControl,bleTxEventHandler

CustomEvents:buttonEventControl,buttonEventHandler

CustomEvents:lcdMainMenuDisplayEventControl,lcdMainMenuDisplayEventHandler

CustomEvents:lcdPermitJoinEventControl,lcdPermitJoinEventHandler

#  If bindings are enabled then this is the maximum number of supported
#  bindings.
NumberOfBindings:2

#  The size of the stack address table which will be used by the stack to
#  maintain IEEE to ZigBee short id mappings.
AddressTableSize:2

#  The size of the portion of the address table used by the trust center as an
#  address cache. The total size of the address table will be equal to this
#  value plus the size of the address table set in the AddressTableSize.
TrustCenterCacheSize:2

#  Manufacturing code user in reporting.
ManufacturingCode:4098

#  Maximum number of supported reported attributes.
ReportTableSize:5

#  The mode of the link key handling on a trust center.
LinkKeyMode:2

#  If not using multiple endpoint support, this value contains the default
#  endpoint. With multiple endpoint support, this number is ignored.
Endpoint:10

#  Version of this device.
DeviceVersion:0

#  Master endpoint which contains global information.
DefaultDestinationEndpoint:10

#  Profile Id used for the application.
ProfileId:-1

#  Device Id used for the application.
DeviceId:-1

#  The largest size for a fragment buffer.
FragmentationMaxSize:255

#  Size of the table for source routing.
SourceRouteTableSize:7

#  Default response policy.
DefaultResponsePolicy:0

#  The level of debugging supported.
DebugLevel:0

#  Configuration of command-line interface.
CLIMode:2

#  If key switching is enabled, this value describes the kind of switch type
#  that the application does.
KeySwitchType:0

#  If key switch is time based, then this value contains the number of seconds
#  between switches.
KeySwitchInterval:604800

#  The type of key generation, random or ping-pong.
KeyGenerationType:0

#  Configuration of heartbeat.
HeartbeatLed:0

#  Configuration of first application button.
FirstButton:1

#  Configuration of second application button.
SecondButton:2

#  If this option is set to true, standard reporting is enabled.
EnableStandardReporting:false

#  If the device needs to perform inter-PAN sends, then this option should be
#  enabled.
EnableInterPanSend:false

#  If the device needs to perform inter-PAN receives, then this option should be
#  enabled.
EnableInterPanReceive:false

#  Enable serial commands for ZDO.
EnableZdoSerialCommands:false

#  Enable this option if you wish to enable device bindings.
EnableBindings:true

#  Turn this option on, if end-device binding is enabled.
EnableEndDeviceBind:false

#  Enables the statistics receiving.
EnableReceiveStatistics:false

#  If true, then command discovery commands are supported.
SupportCommandDiscovery:true

#  Selects whether application will use the ECC 163k1 library.
UseEcc163k1:false

#  Selects whether application will use the ECC 283k1 library.
UseEcc283k1:false

#  Enable preconfigured keys for security.
PreconfiguredKeyEnabled:false

#  Enable network key.
NetworkKeyEnabled:false

#  If this option is turned on, then appBuilder will automatically generate the
#  files, immediately upon saving the ISC file.
AutoGenerate:false

#  Enable key switching.
EnableKeySwitch:false

#  Use this setting to turn on fragmentation.
FragmentationEnable:false

#  Enables concentrator support
EnableConcentrator:false

#  If true, then this concentrator is low ram, otherwise high ram
LowRamConcentrator:true

#  If this option is set to true, then MFG_INSTALL_CODE token is used for
#  setting the security install code.
UseSeInstallCodes:false

#  If this option is turned on, then the code will enable the checking of the
#  attributes.
EnableAttributeRangeChecking:false

#  Enable application handling of supported ZigBee Device Object messages.
ReceiveSupportedZdoRequests:false

#  Enable application handling of unsupported ZigBee Device Object messages.
HandleUnsupportedZdoRequests:false

#  Enable application handling of ZigBee Device Object requests related to
#  endpoints.
HandleEndpointZdoRequests:false

#  Enable application handling of ZigBee Device Object requests related to
#  bindings.
HandleBindingZdoRequests:false

#  Use token for TX power mode.
TxPowerModeUseToken:true

#  Enable boost power mode.
BoostMode:false

#  Enable the alternate transmitter output.
AlternatePowerMode:false

#  Use legacy CLI instead of generated CLI.
LegacyCli:false

#  Add Custom CLI sub-menu
AddCustomCli:true

#  Include command and argument descriptions in the embedded code.
IncludeCommandDescriptions:true

#  If set, then project-specific callbacks file will be generated.
GenerateCallbacksFile:false

#  The manufacturer code for this app defaults to 0.
ManufacturerCodeDefaultIsZero:true

#  Actual preconfigured key, if it is enabled.
PreconfiguredKey:56777777777777777777777777777777

#  Actual network key.
NetworkKey:12333333333333333333333333333333

#  Actual second network key.
NetworkKey2:ABCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC


# Setup configurations
{setupId:additionalFiles
}
{setupId:bleGattConfigurator
<?xml version="1.0" encoding="UTF-8"?><gatt generic_attribute_service="true" header="gatt_db.h" name="Custom BLE GATT" out="gatt_db.c" prefix="gattdb_">
  <service advertise="false" id="device_information" name="Device Information" requirement="mandatory" sourceId="org.bluetooth.service.device_information" type="primary" uuid="180A">
    <informativeText>Abstract: The Device Information Service exposes manufacturer and/or vendor information about a device. Summary: This service exposes manufacturer information about a device. The Device Information Service is instantiated as a Primary Service. Only one instance of the Device Information Service is exposed on a device. </informativeText>
    <characteristic id="manufacturer_name_string" name="Manufacturer Name String" sourceId="org.bluetooth.characteristic.manufacturer_name_string" uuid="2A29">
      <informativeText>Abstract: The value of this characteristic is a UTF-8 string representing the name of the manufacturer of the device. </informativeText>
      <value length="12" type="utf-8" variable_length="true">Silicon Labs</value>
      <properties indicate="false" indicate_requirement="excluded" notify="false" notify_requirement="excluded" read="true" read_requirement="mandatory" reliable_write="false" reliable_write_requirement="excluded" write="false" write_no_response="false" write_no_response_requirement="excluded" write_requirement="excluded"/>
    </characteristic>
    <characteristic id="model_number_string" name="Model Number String" sourceId="org.bluetooth.characteristic.model_number_string" uuid="2A24">
      <informativeText>Abstract: The value of this characteristic is a UTF-8 string representing the model number of the device. </informativeText>
      <value length="8" type="utf-8" variable_length="false">DMP-001A</value>
      <properties indicate="false" indicate_requirement="excluded" notify="false" notify_requirement="excluded" read="true" read_requirement="mandatory" reliable_write="false" reliable_write_requirement="optional" write="false" write_no_response="false" write_no_response_requirement="excluded" write_requirement="excluded"/>
    </characteristic>
    <characteristic id="serial_number_string" name="Serial Number String" sourceId="org.bluetooth.characteristic.serial_number_string" uuid="2A25">
      <informativeText>Abstract: The value of this characteristic is a UTF-8 string representing the serial number of the device. </informativeText>
      <value length="3" type="utf-8" variable_length="false">001</value>
      <properties indicate="false" indicate_requirement="excluded" notify="false" notify_requirement="excluded" read="true" read_requirement="mandatory" reliable_write="false" reliable_write_requirement="excluded" write="false" write_no_response="false" write_no_response_requirement="excluded" write_requirement="excluded"/>
    </characteristic>
    <characteristic id="firmware_revision_string" name="Firmware Revision String" sourceId="org.bluetooth.characteristic.firmware_revision_string" uuid="2A26">
      <informativeText>Abstract: The value of this characteristic is a UTF-8 string representing the firmware version of the device. </informativeText>
      <value length="5" type="utf-8" variable_length="false">0.0.1</value>
      <properties indicate="false" indicate_requirement="excluded" notify="false" notify_requirement="excluded" read="true" read_requirement="mandatory" reliable_write="false" reliable_write_requirement="excluded" write="false" write_no_response="false" write_no_response_requirement="excluded" write_requirement="excluded"/>
    </characteristic>
  </service>
  <service advertise="false" id="device_information" name="Generic Access" requirement="mandatory" sourceId="org.bluetooth.service.generic_access" type="primary" uuid="1800">
    <informativeText>Abstract: The generic_access service contains generic information about the device. All available Characteristics are readonly. </informativeText>
    <characteristic id="device_name" name="Device Name" sourceId="org.bluetooth.characteristic.gap.device_name" uuid="2A00">
      <informativeText/>
      <value length="8" type="utf-8" variable_length="true">DMP Demo</value>
      <properties indicate="false" indicate_requirement="excluded" notify="false" notify_requirement="excluded" read="true" read_requirement="mandatory" reliable_write="false" reliable_write_requirement="excluded" write="false" write_no_response="false" write_no_response_requirement="excluded" write_requirement="optional"/>
    </characteristic>
    <characteristic id="appearance" name="Appearance" sourceId="org.bluetooth.characteristic.gap.appearance" uuid="2A01">
      <informativeText/>
      <value length="2" type="hex" variable_length="false"/>
      <properties indicate="false" indicate_requirement="excluded" notify="false" notify_requirement="excluded" read="true" read_requirement="mandatory" reliable_write="false" reliable_write_requirement="excluded" write="false" write_no_response="false" write_no_response_requirement="excluded" write_requirement="excluded"/>
    </characteristic>
  </service>
  <service advertise="false" name="Silabs DMP LightSED" requirement="mandatory" type="primary" uuid="bae55b96-7d19-458d-970c-50613d801bc9">
    <informativeText/>
    <characteristic id="light_state" name="Light" sourceId="custom.type" uuid="76e137ac-b15f-49d7-9c4c-e278e6492ad9">
      <informativeText/>
      <value length="1" type="user" variable_length="false">0x00</value>
      <properties indicate="true" indicate_requirement="optional" read="true" read_requirement="optional" write="true" write_requirement="optional"/>
    </characteristic>
    <characteristic id="trigger_source" name="Trigger Source" sourceId="custom.type" uuid="2f16ee52-0bfd-4597-85d4-a5141fdbae15">
      <informativeText/>
      <value length="1" type="user" variable_length="false">0x00</value>
      <properties indicate="true" indicate_requirement="optional" read="true" read_requirement="optional" write="true" write_requirement="optional"/>
    </characteristic>
    <characteristic id="source_address" name="Source Address" sourceId="custom.type" uuid="82a1cb54-3921-4c9c-ba34-34f78bab9a1b">
      <informativeText/>
      <value length="8" type="user" variable_length="false">0x00</value>
      <properties indicate="true" indicate_requirement="optional" read="true" read_requirement="optional"/>
    </characteristic>
  </service>
</gatt>
}
{setupId:boardHeader
allowMissingHeader:false
useHeaderInPlace:false
efr32~family[M]~series[1]~device_configuration[2]~performance[P]~radio[332]~flash[1024K]~temp[G]~package[L]~pins[125]+BRD4162A+iar=USE_HARDWARE_CONFIGURATOR,,,
}
{setupId:bookkeeping
}
{setupId:bootloader
em357=application,
efr32~series[1]~device_configuration[1]=application,
efr32~series[1]~device_configuration[2]=application,
efr32~series[1]~device_configuration[3]=application,
efr32~series[1]~device_configuration[4]=application,
}
{setupId:callbackConfiguration
}
{setupId:debugConfiguration
on
area name off
appSerial=1
compile,OTA_BOOTLOAD_CLUSTER
enable,OTA_BOOTLOAD_CLUSTER
}
{setupId:halOptions
}
{setupId:hwConfig
featureLevel=1
active=true
}
{setupId:information
\{key:description
Sample application demonstrating a Sleepy light application using dynamic
multiprotocol (ZigBee + BLE).

The Dynamic Multiprotocol Demo LightSED application demonstrate the dynamic
multiprotocol feature from Silabs. In particular, these applications
demonstrate the ZigBee and BLE stacks running concurrently as MicriumOS tasks.

The Demo is set up to run on the WSTK6000B Mesh Development Kit. The Demo makes
use of the LCD display, LEDs and Buttons on the WSTK.

The Light is configured as a ZigBee Sleepy End Device (SED) and searches for a 
a Network to join. A help screen is shown on the LCD display to assist
the user to join and control the Light. A complementary
application named DynamicMultiprotocolDemoSwitchSoc is available to run on a
WSTK board and join the network formed by the Light and control the state of
LightSED via buttons on the WSTK running the Switch application.

On the BLE interface the Light is setup to advertise itself using Eddystone and
iBeacon in an alternate manner. The Light advertises itself as available for a
connection by a smartphone running Wireless Gecko application. Once connected
the user can control the Light (represented by LEDs on the WSTK board) using
Wireless Gecko smartphone application.

A change in the Light state initiated by the either the smartphone over the BLE
connection or via the zigbee only Switch is propagated to connected device over
both the zigbee and BLE interface.

All application code is contained in the _callbacks.c files within each
application directory.

To use each application:

   1. Load the included application configuration file (i.e., the .isc file)
      into Simplicity Studio.

   2. Enter a new name for the application in the pop-up window.

   3. Generate the application's header and project/workspace files by
      clicking on the "Generate" button in Simplicity Studio.  The application
      files will be generated in the app/builder/<name> directory in the stack
      installation location.

   4. Load the generated project file into the appropriate compiler and build
      the project.

   5. Load the binary image onto a device using Simplicity Studio.
\}
}
{setupId:macros
EMBER_END_DEVICE_POLL_TIMEOUT=225
EMBER_END_DEVICE_POLL_TIMEOUT_SHIFT=6
-DDISABLE_WATCHDOG
-DEMBER_RETRY_QUEUE_SIZE=29
-DEMBER_QA
-DDEVICE_TYPE=2
-DNO_LED=1
}
{setupId:mpsi
- mappings
- custom messages
}
{setupId:quizz
}
{setupId:rf4ce
nodeCapabilities=0
vendorId=65521
vendorString=
userString=
deviceTypes=[254]
profileIds=[0]
power=3
}
{setupId:rf4ceMso
}
{setupId:rf4ceZrc
}
{setupId:serial
useHwConfigurator=true
}
{setupId:template
}
{setupId:token
}
#  The name of the set of Command Line Interface (CLI) commands that are
#  compiled into the application by default.
CliCommandSet:Full

#  These are the various Command Line Interface (CLI) commands that can be
#  included, or excluded (if they are included by default), in the application.
CliCommands:compile,plugin counter print-counter-type

CliCommands:compile,plugin counters clear

CliCommands:compile,plugin counters print

CliCommands:compile,plugin counters print-thresholds

CliCommands:compile,plugin counters reset-threshold

CliCommands:compile,plugin counters send-request

CliCommands:compile,plugin counters set-threshold

CliCommands:compile,plugin counters simple-print

CliCommands:compile,plugin find-and-bind initiator

CliCommands:compile,plugin find-and-bind target

CliCommands:compile,plugin fragmentation artificial-block-drop

CliCommands:compile,plugin fragmentation set-rx-window-size

CliCommands:compile,plugin mn-price-passthrough print

CliCommands:compile,plugin mn-price-passthrough set-routing

CliCommands:compile,plugin mn-price-passthrough start

CliCommands:compile,plugin mn-price-passthrough stop

CliCommands:compile,plugin network-creator form

CliCommands:compile,plugin network-creator mask add

CliCommands:compile,plugin network-creator mask set

CliCommands:compile,plugin network-creator mask subtract

CliCommands:compile,plugin network-creator start

CliCommands:compile,plugin network-creator status

CliCommands:compile,plugin network-creator stop

CliCommands:remove,plugin ota-storage-common data-print

CliCommands:remove,plugin ota-storage-common delete

CliCommands:remove,plugin ota-storage-common printImages

CliCommands:remove,plugin ota-storage-common reload

CliCommands:remove,plugin ota-storage-common storage-info

CliCommands:remove,plugin ota-storage-eeprom wipe

#  Plugin configuration
appPlugin:adc,true

appPlugin:address-table,true

appPlugin:aes-cmac,false

appPlugin:antenna,false

appPlugin:antenna-stub,true

appPlugin:barrier-control-server,false

appPlugin:basic,false

appPlugin:battery-monitor,false

appPlugin:battery-monitor-stub,false

appPlugin:binding-table-library,true

appPlugin:ble,true

appPlugin:ble-psstore-library,true

appPlugin:bulb-pwm-cli,false

appPlugin:bulb-pwm-driver,false

appPlugin:bulb-ui,false

appPlugin:button-interface,false

appPlugin:button-interface-stub,false

appPlugin:button-joining,false

appPlugin:calendar-client,false

appPlugin:calendar-common,false

appPlugin:calendar-server,false

appPlugin:cbke-163k1-library,false

appPlugin:cbke-283k1-library,false

appPlugin:cbke-library-core,false

appPlugin:cbke-library-dsa-sign,false

appPlugin:cbke-library-dsa-verify,false

appPlugin:cbke-library-dsa-verify-283k1,false

appPlugin:cjson,false

appPlugin:coexistence,true

appPlugin:color-control,false

appPlugin:color-control-server,false

appPlugin:command-relay,false

appPlugin:comms-hub-function,false

appPlugin:comms-hub-function-sub-ghz,false

appPlugin:concentrator,false

appPlugin:configuration-server,false

appPlugin:connection-manager,false

appPlugin:counters,true

appPlugin:debug-basic-library,true

appPlugin:debug-extended-library,false

appPlugin:debug-jtag,false

appPlugin:debug-jtag-stub,true

appPlugin:device-database,false

appPlugin:device-management-client,false

appPlugin:device-management-server,false

appPlugin:device-query-service,false

appPlugin:device-table,false

appPlugin:diagnostic-server,false

appPlugin:dmp-demo-ui,false

appPlugin:dmp-ui-demo,true

appPlugin:dmp-ui-demo-stub,false

appPlugin:door-lock-server,false

appPlugin:drlc,false

appPlugin:drlc-server,false

appPlugin:ecc-library-163k1,false

appPlugin:ecc-library-283k1,false

appPlugin:eeprom,true

appPlugin:eeprom-powerdown,false

appPlugin:electrical-measurement-server,false

appPlugin:em4,false

appPlugin:ember-minimal-printf,true

appPlugin:end-device-bind-library,false

appPlugin:end-device-support,true

appPlugin:esi-management,false

appPlugin:events-client,false

appPlugin:events-server,false

appPlugin:ezmode-commissioning,false

appPlugin:fem-control,false

appPlugin:find-and-bind-initiator,false

appPlugin:find-and-bind-target,true

appPlugin:form-and-join,false

appPlugin:fragmentation,false

appPlugin:gas-proxy-function,false

appPlugin:gbcs-compatibility,false

appPlugin:gbcs-device-log,false

appPlugin:gbcs-gas-meter,false

appPlugin:gbz-message-controller,false

appPlugin:general-response-commands,false

appPlugin:generic-interrupt-control,false

appPlugin:generic-interrupt-control-stub,false

appPlugin:glib,true

appPlugin:gp-library,false

appPlugin:gpio-sensor,false

appPlugin:gpio-sensor-stub,false

appPlugin:green-power-client,false

appPlugin:green-power-common,false

appPlugin:green-power-server,false

appPlugin:green-power-test-device,false

appPlugin:groups-client,false

appPlugin:groups-server,true

appPlugin:hal-library,true

appPlugin:hc-11073-tunnel,false

appPlugin:heartbeat,false

appPlugin:humidity-si7021,false

appPlugin:humidity-si7021-stub,false

appPlugin:i2c-driver,false

appPlugin:i2c-driver-stub,false

appPlugin:ias-zone-client,false

appPlugin:ias-zone-server,false

appPlugin:identify,true

appPlugin:identify-feedback,false

appPlugin:idle-sleep,true

appPlugin:illuminance-measurement-server,false

appPlugin:illuminance-si1141,false

appPlugin:illuminance-si1141-stub,false

appPlugin:install-code-library,true

appPlugin:interpan,true

appPlugin:key-establishment,false

appPlugin:led-blink,false

appPlugin:led-blink-stub,false

appPlugin:led-dim-pwm,false

appPlugin:led-rgb-pwm,false

appPlugin:led-temp-pwm,false

appPlugin:level-control,true

appPlugin:libcoap,false

appPlugin:linked-list,false

appPlugin:low-voltage-shutdown,false

appPlugin:mac-address-filtering,false

appPlugin:manufacturing-library,false

appPlugin:manufacturing-library-cli,false

appPlugin:manufacturing-library-ota,false

appPlugin:mbedtls,true

appPlugin:messaging-client,false

appPlugin:messaging-server,false

appPlugin:meter-mirror,false

appPlugin:meter-snapshot-client,false

appPlugin:meter-snapshot-server,false

appPlugin:meter-snapshot-storage,false

appPlugin:metering-server,false

appPlugin:micrium-rtos,true

appPlugin:mn-price-passthrough,false

appPlugin:mpsi,false

appPlugin:mpsi-ipc,false

appPlugin:mpsi-storage,false

appPlugin:multi-network-library,false

appPlugin:network-creator,false

appPlugin:network-creator-security,false

appPlugin:network-find,false

appPlugin:network-find-sub-ghz,false

appPlugin:network-steering,true

appPlugin:nvm3,false

appPlugin:occupancy-pyd1698,false

appPlugin:occupancy-pyd1698-cli,false

appPlugin:occupancy-pyd1698-stub,false

appPlugin:occupancy-sensor-server,false

appPlugin:on-off,true

appPlugin:ota-bootload,false

appPlugin:ota-client,false

appPlugin:ota-client-policy,false

appPlugin:ota-common,false

appPlugin:ota-server,false

appPlugin:ota-server-policy,false

appPlugin:ota-storage-common,false

appPlugin:ota-storage-posix-filesystem,false

appPlugin:ota-storage-simple,false

appPlugin:ota-storage-simple-eeprom,false

appPlugin:ota-storage-simple-ram,false

appPlugin:packet-validate-library,true

appPlugin:paho.mqtt.c,false

appPlugin:partner-link-key-exchange,false

appPlugin:permit-join-manager,false

appPlugin:poll-control-client,false

appPlugin:poll-control-server,false

appPlugin:power-configuration-server,false

appPlugin:power-consumption-model,false

appPlugin:power-meter-cs5463,false

appPlugin:power-meter-cs5463-stub,false

appPlugin:prepayment-client,false

appPlugin:prepayment-server,false

appPlugin:prepayment-snapshot-storage,false

appPlugin:price-client,false

appPlugin:price-common,false

appPlugin:price-server,false

appPlugin:psstore,false

appPlugin:rail-library,false

appPlugin:rail-library-mp,true

appPlugin:relative-humidity-measurement-server,false

appPlugin:reporting,true

appPlugin:sb1-gesture-sensor,false

appPlugin:sb1-gesture-sensor-stub,false

appPlugin:scan-dispatch,true

appPlugin:scenes,true

appPlugin:scenes-client,false

appPlugin:security-library-core,true

appPlugin:security-link-keys-library,false

appPlugin:security-sensor,false

appPlugin:serial,true

appPlugin:silabs-device-ui,false

appPlugin:sim-eeprom1,true

appPlugin:sim-eeprom2,false

appPlugin:sim-eeprom2-1to2-upgrade,false

appPlugin:sim-eeprom2-1to2-upgrade-stub,false

appPlugin:sim-eeprom2-to-nvm3-upgrade,false

appPlugin:sim-eeprom2-to-nvm3-upgrade-stub,false

appPlugin:simple-clock,false

appPlugin:simple-main,false

appPlugin:simple-metering-client,false

appPlugin:simple-metering-server,false

appPlugin:sleepy-message-queue,false

appPlugin:slot-manager,false

appPlugin:smart-energy-registration,false

appPlugin:stack-diagnostics,false

appPlugin:standalone-bootloader-client,false

appPlugin:standalone-bootloader-common,false

appPlugin:standalone-bootloader-server,false

appPlugin:standard-printf-support,false

appPlugin:sub-ghz-client,false

appPlugin:sub-ghz-server,false

appPlugin:tamper-switch,false

appPlugin:tamper-switch-stub,false

appPlugin:temperature-measurement-server,false

appPlugin:temperature-si7021,false

appPlugin:temperature-si7053,false

appPlugin:temperature-si7053-stub,false

appPlugin:test-harness,false

appPlugin:test-harness-z3,false

appPlugin:throughput,false

appPlugin:time-server,false

appPlugin:transport-mqtt,false

appPlugin:trust-center-backup,false

appPlugin:trust-center-keepalive,false

appPlugin:trust-center-nwk-key-update-broadcast,false

appPlugin:trust-center-nwk-key-update-periodic,false

appPlugin:trust-center-nwk-key-update-unicast,false

appPlugin:tunneling-client,false

appPlugin:tunneling-server,false

appPlugin:update-ha-tc-link-key,false

appPlugin:update-tc-link-key,true

appPlugin:wstk-display,true

appPlugin:xmodem-sender,false

appPlugin:zigbee-pro-bc-table-mbedtls-library,false

appPlugin:zigbee-pro-leaf-library,true

appPlugin:zigbee-pro-library,false

appPlugin:zigbee-r22-support-library,false

appPlugin:zll-commissioning,false

appPlugin:zll-identify-server,true

appPlugin:zll-level-control-server,false

appPlugin:zll-library,true

appPlugin:zll-on-off-server,true

appPlugin:zll-scenes-client,false

appPlugin:zll-scenes-server,true

appPlugin:zll-utility-client,false

appPlugin:zll-utility-server,false

#  Plugin specific options
AppPluginOption:EMBER_AF_PLUGIN_INTERPAN_ALLOW_REQUIRED_SMART_ENERGY_MESSAGES,false

AppPluginOption:EMBER_AF_PLUGIN_ZLL_COMMISSIONING_LINK_INITIATOR,false

AppPluginOption:EMBER_AF_PLUGIN_ZLL_COMMISSIONING_TOUCH_LINK_SECONDS_DELAY,3

AppPluginOption:EMBER_AF_PLUGIN_ZLL_COMMISSIONING_SUB_DEVICE_TABLE_SIZE,1

AppPluginOption:EMBER_AF_PLUGIN_ZLL_COMMISSIONING_SCAN_POWER_LEVEL,0

AppPluginOption:EMBER_AF_PLUGIN_ZLL_COMMISSIONING_IDENTIFY_DURATION,65535

AppPluginOption:EMBER_AF_PLUGIN_IDLE_SLEEP_STAY_AWAKE_WHEN_NOT_JOINED,true

AppPluginOption:EMBER_AF_PLUGIN_MICRIUM_RTOS_POLL_CLI,true

AppPluginOption:EMBER_AF_PLUGIN_MICRIUM_RTOS_SLEEP_ENABLE,true

AppPluginOption:EMBER_AF_PLUGIN_BLE_MAX_CONNECTIONS,5

AppPluginOption:EMBER_BROADCAST_TABLE_SIZE,35

AppPluginOption:EMBER_AF_PLUGIN_OTA_CLIENT_POLICY_IMAGE_TYPE_ID,4

AppPluginOption:EMBER_AF_PLUGIN_OTA_CLIENT_POLICY_FIRMWARE_VERSION,2

AppPluginOption:EMBER_AF_PLUGIN_OTA_STORAGE_SIMPLE_EEPROM_STORAGE_END,524288

AppPluginOption:EMBER_AF_PLUGIN_END_DEVICE_SUPPORT_LONG_POLL_INTERVAL_SECONDS,4

AppPluginOption:EMBER_AF_PLUGIN_END_DEVICE_SUPPORT_ENHANCED_SLEEP_SUPPORT,false

AppPluginOption:EMBER_AF_PLUGIN_IDENTIFY_FEEDBACK_LED_FEEDBACK,false

AppPluginOption:EMBER_AF_PLUGIN_END_DEVICE_SUPPORT_LONG_POLL_INTERVAL_SECONDS,5

AppPluginOption:EMBER_AF_REJOIN_ATTEMPTS_MAX,255

AppPluginOption:EMBER_AF_PLUGIN_NETWORK_STEERING_CHANNEL_MASK,0x02108800

AppPluginOption:EMBER_AF_PLUGIN_END_DEVICE_SUPPORT_ENHANCED_SLEEP_SUPPORT,true

